- Top
- Shooting
- Basic procedures
- Adjustments for shooting

# Adjustments for shooting

For shooting, use the following steps.

Switch the <CC FILTER>/<ND FILTER> dial setting according to the light conditions.

For details on setting example of the <CC FILTER>/<ND FILTER> dial, refer to “Shooting and recording (Camera unit)”.

Operate the <WHITE BAL> switch.

#### When white balance is already saved in memory

- Set the <WHITE BAL> switch to <A> or <B>.

#### When neither white or black balance is saved in memory and there is no time to adjust the white balance:

- Set the <WHITE BAL> switch to <PRST>. The white balance matched to the filter is automatically adjusted according to the <CC FILTER>/<ND FILTER> dial setting.

#### When adjusting the white balance on the spot

- Select the filter matched to the lighting conditions. Set the <WHITE BAL> switch to <A> or <B>, shoot a white subject in the center of the screen, and follow the steps below to adjust the white balance.

Press the <AUTO W/B BAL> switch towards the <AWB> side to adjust the white balance. (White balance adjustment)

Press the <AUTO W/B BAL> switch towards the <ABB> side to adjust the black balance. (Black balance adjustment)

Press the <AUTO W/B BAL> switch towards the <AWB> side to re-adjust the white balance.

Point the camera at the subject and adjust the focus and zoom.

When using the electronic shutter, set the shutter mode and shutter speed. (Setting the electronic shutter)

NOTE

- When highly bright subjects (e.g. sun or lighting) are shot, the periphery of the subject might be colored.

Top of the page