- Top
- Playback
- Thumbnail operation
- Copying clips

# Copying clips

Clips can be copied between memory cards.

Only the clip recorded in P2 can be copied.

[ALL SLOT]

[COPY]

[ALL SLOT]

[COPY]

[EXIT]

[EXIT]

[EXIT]

[THUMBNAIL]

[EXIT]

[EXIT]

[THUMBNAIL]

[EXIT]

[EXIT]

[ALL]

[AUDIO]

[PROTECT]

[PLAYBACK]

[PLAYBACK]

[ALL]

[SLOT1→SLOT2]

[AUDIO]

[PROTECT]

[DELETE]

[VIDEO OUT/LCD/VF]

[VIDEO OUT/LCD/VF]

[SELECT]

[CLIP]

[DELETE]

[SLOT1→SLOT3]

[CLIP]

[SELECT]

[SLOT2→SLOT1]

[DISPLAY]

[RECORDING]

[COPY]

[COPY]

[RECORDING]

[DISPLAY]

[REPAIR]

[NETWORK]

[SLOT2→SLOT3]

[REPAIR]

[NETWORK]

[SYSTEM]

[SLOT3→SLOT1]

[SYSTEM]

[SLOT3→SLOT2]

[OTHERS]

[INFORMATION]

[INFORMATION]

[OTHERS]

Fig. 1

Fig. 2

[SLOT1→SLOT2]

[COPY]

[SLOT1→SLOT2]

[COPY]

Fig. 3

Fig. 4

[SLOT1→SLOT2]

[COPY]

[COPY]

[COPY] completed.

Fig. 5

Press the <THUMBNAIL> button.

The thumbnail screen is displayed.

Press the <MENU> button while the thumbnail screen is displayed.

The menu is displayed.

Select the [THUMBNAIL] menu → [CLIP] → [COPY].

Select [SELECT]. (Fig. 1)

- All clips can be copied between the memory cards when [ALL] is selected.

Select the card slot for the copy destination. (Fig. 2)

The clips on the memory card of the copy source is displayed in the thumbnail screen. (Fig. 3)

- [SLOT1→SLOT2]: Copies clips from the memory card in card slot 1 to the memory card in card slot 2.

- [SLOT1→SLOT3]: Copies clips from the memory card in card slot 1 to the memory card in card slot 3.

- [SLOT2→SLOT1]: Copies clips from the memory card in card slot 2 to the memory card in card slot 1.

- [SLOT2→SLOT3]: Copies clips from the memory card in card slot 2 to the memory card in card slot 3.

- [SLOT3→SLOT1]: Copies clips from the memory card in card slot 3 to the memory card in card slot 1.

- [SLOT3→SLOT2]: Copies clips from the memory card in card slot 3 to the memory card in card slot 2.

Select the clip to copy in the thumbnail screen.

is displayed on the selected clip.

Select . (Fig. 4)

- This can also be selected by pressing and holding the jog dial button.

When the confirmation message is displayed, select [SET].

Progress bar is displayed, and the copy of the clip starts.

[OVERWRITE?] is displayed when there is a same P2 clip in the copy destination. Select [SET] when overwriting the clip, and select when not overwriting the clip.

- To cancel the copy midway, select [CANCEL].

When the completion message is displayed, select . (Fig. 5)

NOTE

- Clips in MOV format cannot be copied.

- The copy is not possible when the volume of the selected clip is larger than the available memory card capacity of the destination.

- The copy is not possible when the copy destination memory card is write protected.

- The copy is not possible when it will exceed the maximum number of clips.

- The P2 clip exceeding 4 GB cannot be copied to a memory card of 32 GB or less.

- The P2 clip recorded over multiple memory cards cannot be copied to a same memory card.

Top of the page