- Top
- Shooting
- Scene file
- Writing and loading lens files to and from SD card

# Writing and loading lens files to and from SD card

Eight lens files stored in the internal memory on the camera can be written to a SD card as a single card file. For lens files written to the SD card, the written single card file (eight lens files) can be loaded into the internal memory.

The following shows the relationship between lens files stored to the internal memory and card files written to the SD card.

Internal memory

eight lens files

Up to eight lens files can be stored in internal memory.

The contents of the eight lens files can be written to and loaded from a SD card as a single card file.

Card file 1

Card file n

## Writing lens files to SD card

[EXIT]

[EXIT]

[CAMERA]

[MENU]>[OTHERS]>[FILE]>[LENS FILE(SD CARD)]>[SAVE]

[EXIT]

[DEC-01-2019]

[SCENE FILE]

[SCENE FILE(SD CARD)]

[LOAD]

[FILE]

[DEC-01-2019]

[AUDIO]

[BATTERY]

[SETUP FILE(SD CARD)]

[SAVE]

[DEC-01-2019]

[VIDEO OUT/LCD/VF]

[SAVE AS]

[GENLOCK]

[SETUP FILE(MEMORY)]

[DEC-01-2019]

[RECORDING]

[COLOR BARS]

[CAC FILE(SD CARD)]

[NETWORK]

[LED]

[LENS FILE(SD CARD)]

[CLOCK]

[SYSTEM]

[LENS FILE(MEMORY)]

[OTHERS]

[GPS]

[SLOT FOR LOAD/SAVE]

Fig. 1

Fig. 2

### Saving a lens file as a new file on a SD card

Current setting values of the camera is saved as a new file in a SD card by specifying the card file name.

Select the [OTHERS] menu → [FILE] → [LENS FILE(SD CARD)] → [SAVE AS].

The card file name entry screen and the keyboard are displayed.

Enter the text to set with the keyboard.

Select [Enter].

A confirmation screen is displayed.

Select [SET].

The card file is saved.

### Overwriting a lens file on a SD card

Overwrites the file selected in the list of the card files saved on the SD card with the current setting values of the camera.

Select the [OTHERS] menu → [FILE] → [LENS FILE(SD CARD)] → [SAVE]. (Fig. 1)

The list of card files saved on the SD card is displayed.

Select the file to overwrite from the list of card files. (Fig. 2)

The card file name entry screen and the keyboard are displayed. Leave it as is when overwriting.

Select [Enter].

A confirmation screen is displayed.

Select [SET].

The card file is saved.

- An error message may be displayed. For error message, refer to “Warning system”.

## Loading lens files from SD card

Select the [OTHERS] menu → [FILE] → [LENS FILE(SD CARD)] → [LOAD].

The list of card files saved on the SD card is displayed.

Select the card file to load.

A confirmation screen is displayed.

Select [SET].

Loading of the file begins.

When the completion message is displayed, press the jog dial button (or <SET> button).

- An error message may be displayed. For error message, refer to “Warning system”.

NOTE

- Titles of lens files included in the card file saved in the SD card are not displayed in the [LENS FILE(SD CARD)] screen. Load the file each time and confirm them in the [LENS FILE(MEMORY)] screen. Lens file in the internal memory will be overwritten when loading the lens file. Backup the lens file in the internal memory by writing it on the SD card before loading a lens file from a SD card.

## CAC file

For details, refer to “Chromatic aberration compensation function (CAC)”.

Top of the page