- Top
- Shooting
- Basic procedures
- Normal recording

# Normal recording

Press the <REC> button to start recording of video and audio on the memory card.

A data consisting of image and sound generated by a single shooting action, together with additional information, is called a “clip”.

Press the <REC> button to start recording.

The [REC] lamp in the viewfinder is illuminated during recording.

Press the <REC> button again to stop.

The [REC] lamp in the viewfinder goes out.

NOTE

- <REV ()>/<STOP ()>/<FWD ()>/<PLAY/PAUSE (/)> buttons will not operate during recording.

- In the following cases, it may take time to complete writing to the memory card.

  Pressing the <REC> button does not accept operations immediately.

  - When short-burst recording is stopped

  - When stopping recording immediately after recording to the second memory card

- The recording is started using the memory of the camera even if the recording is started right after the memory card is inserted or the power is turned on. In such case, the recording cannot be stopped until the memory card is recognized. The warning is displayed as [REC PAUSE INVALID] at this time.

Top of the page