- Top
- Shooting
- Basic procedures
- Switch settings for shooting

# Switch settings for shooting

After turning on the power and inserting a memory card, set the switches as follows.

1. <GAIN> switch

   Normally, set this to <L> (0 dB). If it is too dark, set the gain to an appropriate value.

2. <OUTPUT>/<AUTO KNEE> switch

   Set this switch to <CAM>/<ON>.

3. <TCG> switch

   Set this switch to <F-RUN> or <R-RUN>.

4. <AUDIO SELECT CH1/3>/<AUDIO SELECT CH2/4> switch

   Set this switch to <AUTO>.

Top of the page