- Top
- Shooting
- Handling setting data
- File structure of the setting data

# File structure of the setting data

The camera has six file data areas.

Factory data | This area stores factory settings. It cannot be rewritten by menu operation.
Current data | This area stores the operation status of the camera. Setting values in this area are changed by menu operation.
Setup file | This area stores values set by menu operation. As default data, factory data is stored here.
Scene file | Six scene files are provided.
Lens files | Eight lens files are provided. Eight of these files can be saved together as a single file on SD card.
CAC file | This area stores 32 chromatic aberration compensation data.

#### Setup file and scene file

Scene file

Setup file

SD card

SD card

[OTHERS] → [FILE] → [SCENE FILE(SD CARD)] → [SAVE]/[SAVE AS]

[OTHERS] → [FILE] → [SCENE FILE(SD CARD)] → [LOAD]

[OTHERS] → [FILE] → [SETUP FILE(SD CARD)] → [SAVE]/[SAVE AS]

[SCENE1] - [SCENE6]

[OTHERS] → [FILE] → [SETUP FILE(SD CARD)] → [LOAD]

[ALL]

Current data

[SCENE FILE] → [LOAD/SAVE/INITIALIZE] → [INITIALIZE]

[SCENE FILE] → [LOAD/SAVE/INITIALIZE] → [LOAD]

[OTHERS] → [FILE] → [SETUP FILE(MEMORY)] → [LOAD]

[OTHERS] → [FILE] → [SETUP FILE(MEMORY)] → [SAVE]

Factory data

[SCENE FILE] → [LOAD/SAVE/INITIALIZE] → [SAVE]

Scene file (memory)

[OTHERS] → [MENU INITIALIZE]

Setup file (memory)

Number of files: 1

Number of files: 6

#### Lens file and CAC file

Current data

Automatically load the file matching with the lens connected by [CAMERA] → [CAC ADJ.] → [CAC CONTROL] → [ON]

[OTHERS] → [FILE] → [LENS FILE(MEMORY)] → [LOAD]

[OTHERS] → [FILE] → [LENS FILE(MEMORY)] → [SAVE]

[OTHERS] → [MENU INITIALIZE]

Lens file (memory)

CAC file (memory)

Factory data

Number of files: 8

Number of files: 32

[OTHERS] → [FILE] → [LENS FILE(SD CARD)] → [SAVE]/[SAVE AS]

[OTHERS] → [FILE] → [CAC FILE(SD CARD)] → [LOAD]

[OTHERS] → [FILE] → [LENS FILE(SD CARD)] → [LOAD]

CAC file

Lens files

SD card

SD card

NOTE

- Each file cannot be operated by displaying the menu during interval recording standby. Press the <REC> or <STOP> button to end interval recording, and try the operation again.

## Setting up using SD cards

An SD card can be used as a setup card that stores menu content.

Use of this data allows you to reproduce optimum setup states.

Top of the page