- Top
- Shooting
- Special recording function
- Interval recording

# Interval recording

The camera will repeat one frame recording at each set interval.

1 frame recording

1 frame recording

1 frame recording

(Time)

Time set in [INTERVAL TIME]

Time set in [INTERVAL TIME]

Select the [RECORDING] menu → [REC FUNCTION] → [REC MODE] → [INTERVAL].

[INTRVL] is displayed in the special recording function display of the camera image screen.

Set the time in the [RECORDING] menu → [REC FUNCTION] → [INTERVAL TIME].

Press the <REC> button.

- [I-REC] is displayed in red in the special recording function display of the camera image screen.

- The camera will repeat one frame recording at each set interval.

- To stop recording, press the <REC> or <STOP> button.

- Set the [RECORDING] menu → [REC FUNCTION] → [REC MODE] → [NORMAL] to clear the setting.

- Set whether to keep the settings after turning off the power in the [RECORDING] menu → [REC FUNCTION] → [REC MODE HOLD].

NOTE

- Audio is not recorded.

- Recorded data (data recorded until recording was stopped) is included in one clip.

- It will be fixed to recording run regardless of the <TCG> switch position when interval recording is enabled.

- The [RECORDING] menu → [TC/UB] → [DF/NDF] is fixed to [NDF].

- [SDI REC REMOTE] and [HDMI REC REMOTE] will not operate.

- If the length of the clip is less than three seconds when the recording is stopped, the image of the final frame will be recorded to make the length of the clip to three seconds.

- The recording is stopped once when the length of the clip exceeds ten hours in the interval recording. The recording is automatically resumed after few seconds.

- For recording limitations of the interval recording, refer to “Recording function that cannot be used simultaneously”.

Top of the page