- Top
- Shooting
- Setting high dynamic range (HDR)
- Recording in high dynamic range (HDR)

# Recording in high dynamic range (HDR)

Select the [SCENE FILE] menu → [GAMMA MODE SEL] → [HLG].

The output will be as follows.

<SDI OUT1> terminal: Outputs in high dynamic range (HDR) or standard dynamic range (SDR) according to the setting of the [VIDEO OUT/LCD/VF] menu → [SDI OUT1] → [SDI OUT HDR].

<SDI OUT2> terminal: Outputs in high dynamic range (HDR) or standard dynamic range (SDR) according to the setting of the [VIDEO OUT/LCD/VF] menu → [SDI OUT2] → [SDI OUT HDR].

<HDMI> terminal: When set to the [VIDEO OUT/LCD/VF] menu → [HDMI OUT] → [SIGNAL SEL] → [SDI OUT1(2160p)], outputs according to the setting of the [VIDEO OUT/LCD/VF] menu → [SDI OUT1] → [SDI OUT HDR]. When set to [SDI OUT2], outputs according to the setting of the [VIDEO OUT/LCD/VF] menu → [SDI OUT2] → [SDI OUT HDR].

Viewfinder, LCD monitor: Outputs according to the setting of the [VIDEO OUT/LCD/VF] menu → [LCD/VF HDR]. HDR or SDR can be selected when recording in HDR.

Top of the page