- Top
- Shooting
- Setting of time data
- How to input user bits

# How to input user bits

By setting user bits, information such as memos (date, time) up to eight digits long (hexadecimal) can be recorded.

Set the <DISPLAY> switch to <UB>.

Set the <TCG> switch to <SET>.

Set the user bits by the cursor operation buttons.

- Screen display

  - : The digit to be set (flashing) moves to the right.

  - : The digit to be set (flashing) moves to the left.

  - : The value of the digit to set (flashing) is incremented by one.

  - : The value of the digit to set (flashing) is decremented by one.

Set the <TCG> switch to <F-RUN> or <R-RUN>.

Set to the [RECORDING] menu → [TC/UB] → [UB MODE] → [USER].

NOTE

- Thumbnail operations and menu operations on thumbnail operation section are not possible while the <TCG> switch is set to <SET>.

## Frame rate information recorded on user bits

Recording the frame rate values for the image information shot/recorded according to the frame rate set in the [SYSTEM] menu → [REC FORMAT] to user bits allows you to use on the editor (personal computer editing software).

### Frame rate information

The relationship between frame rate, image pull-down, time code, and user bits is as follows.

Verification information on the right-hand six digits

REC mark

Fixed values

Frame rate

Camera video mode

#### Camera video mode

The display of the camera video mode differs depending on the setting of following menus.

[FREQUENCY] | Recording frame frequency of [REC FORMAT] | Display of frame rate | Display of camera video mode
--- | --- | --- | ---
[59.94Hz] | 23.98p | 024 | C
| 29.97p | 030 | 8
| 59.94p | 060 | 8
| 59.94i | 060 | 0
[50.00Hz] | 25.00p | 025 | A
| 50.00p | 050 | A
| 50.00i | 050 | 2

Top of the page