- Top
- Operation
- Menu settings
- [AUDIO] menu

# [AUDIO] menu

Sets the input/output function of audio.

## [INPUT SETTINGS]

### [FRONT MIC POWER]

Sets the phantom power supply of the front microphone.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [REAR MIC POWER]

Sets the phantom power supply of the rear microphone.

When [OFF] is selected, the phantom power supply is not output even if the microphone input power selector switch is set to <+48V>.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [FRONT MIC LEVEL]

Sets the input level of the external microphone connected to the front <MIC IN> terminal of the camera.

This is enabled only when an external microphone is connected to the <MIC IN> terminal.

The items that can be set are as follows.

- [−40dB], [−50dB], [−60dB]

(Factory setting: [−40dB])

### [REAR MIC CH1/3 LEVEL]

Sets the audio input level of the external microphone connected to the rear <AUDIO IN CH1/3> terminal of the camera.

This is enabled only when the <LINE>/<MIC> selector switch is set to <MIC>.

The items that can be set are as follows.

- [−40dB], [−50dB], [−60dB]

(Factory setting: [−60dB])

### [REAR MIC CH2/4 LEVEL]

Sets the audio input level of the external microphone connected to the rear <AUDIO IN CH2/4> terminal of the camera.

This is enabled only when the <LINE>/<MIC> selector switch is set to <MIC>.

The items that can be set are as follows.

- [−40dB], [−50dB], [−60dB]

(Factory setting: [−60dB])

### [REAR LINE IN LEVEL]

Sets the audio input level of the device connected to the rear <AUDIO IN CH1/3>/<AUDIO IN CH2/4> terminal of the camera.

This is enabled only when the <LINE>/<MIC> selector switch is set to <LINE>.

The items that can be set are as follows.

- [−3dB], [0dB], [4dB]

(Factory setting: [4dB] (when [AREA SETTINGS] is [AREA 1]/[AREA 2]/[AREA 4]), [0dB] (when [AREA SETTINGS] is [AREA 3]))

### [WIRELESS WARN]

Selects whether to display a warning when the reception status of the wireless microphone receiver is poor.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [WIRELESS TYPE]

Selects the type of wireless microphone receiver.

[SINGLE] | Selects a single channel type wireless microphone receiver.
[DUAL] | Selects a double channel type wireless microphone receiver.

(Factory setting: [SINGLE])

## [REC CH SETTINGS]

### [VOL. SELECT]

Selects which audio channel to assign to the <AUDIO LEVEL CH1/3>/<AUDIO LEVEL CH2/4> dial and the <F.AUDIO LEVEL> dial.

[CH1/2] | Assigns level adjustment of the audio channels 1 and 2. Audio channels 3 and 4 can be automatically adjusted or adjusted by [CH3 LEVEL CONTROL] or [CH4 LEVEL CONTROL].
[CH3/4] | Assigns level adjustment of the audio channels 3 and 4. Audio channels 1 and 2 can be automatically adjusted or adjusted by [CH1 LEVEL CONTROL] or [CH2 LEVEL CONTROL].

(Factory setting: [CH1/2])

### [FRONT VOL. CH1]

Selects if the <F.AUDIO LEVEL> dial is enabled against the audio signal input to the audio channel 1.

[FRONT] | This is enabled when the <AUDIO IN CH1> switch is set to <FRONT>.
[W.L.] | This is enabled when the <AUDIO IN CH1> switch is set to <W.L.>.
[REAR] | This is enabled when the <AUDIO IN CH1> switch is set to <REAR>.
[ALL] | The <F.AUDIO LEVEL> dial is enabled regardless of the setting of the <AUDIO IN CH1> switch.
[OFF] | The <F.AUDIO LEVEL> dial is disabled regardless of the setting of the <AUDIO IN CH1> switch.

(Factory setting: [OFF])

### [FRONT VOL. CH2]

Selects if the <F.AUDIO LEVEL> dial is enabled against the audio signal input to the audio channel 2.

[FRONT] | This is enabled when the <AUDIO IN CH2> switch is set to <FRONT>.
[W.L.] | This is enabled when the <AUDIO IN CH2> switch is set to <W.L.>.
[REAR] | This is enabled when the <AUDIO IN CH2> switch is set to <REAR>.
[ALL] | The <F.AUDIO LEVEL> dial is enabled regardless of the setting of the <AUDIO IN CH2> switch.
[OFF] | The <F.AUDIO LEVEL> dial is disabled regardless of the setting of the <AUDIO IN CH2> switch.

(Factory setting: [OFF])

### [FRONT VOL. CH3]

Selects if the <F.AUDIO LEVEL> dial is enabled against the audio signal input to the audio channel 3.

[FRONT] | This is enabled when the <AUDIO IN CH3> switch is set to <FRONT>.
[W.L.] | This is enabled when the <AUDIO IN CH3> switch is set to <W.L.>.
[REAR] | This is enabled when the <AUDIO IN CH3> switch is set to <REAR>.
[ALL] | The <F.AUDIO LEVEL> dial is enabled regardless of the setting of the <AUDIO IN CH3> switch.
[OFF] | The <F.AUDIO LEVEL> dial is disabled regardless of the setting of the <AUDIO IN CH3> switch.

(Factory setting: [OFF])

### [FRONT VOL. CH4]

Selects if the <F.AUDIO LEVEL> dial is enabled against the audio signal input to the audio channel 4.

[FRONT] | This is enabled when the <AUDIO IN CH4> switch is set to <FRONT>.
[W.L.] | This is enabled when the <AUDIO IN CH4> switch is set to <W.L.>.
[REAR] | This is enabled when the <AUDIO IN CH4> switch is set to <REAR>.
[ALL] | The <F.AUDIO LEVEL> dial is enabled regardless of the setting of the <AUDIO IN CH4> switch.
[OFF] | The <F.AUDIO LEVEL> dial is disabled regardless of the setting of the <AUDIO IN CH4> switch.

(Factory setting: [OFF])

### [CH1 LEVEL]

Select auto/manual for the method to adjust the recording level of the audio channel 1.

The items that can be set are as follows.

- [AUTO], [MANUAL]

(Factory setting: [AUTO])

### [CH2 LEVEL]

Select auto/manual for the method to adjust the recording level of the audio channel 2.

The items that can be set are as follows.

- [AUTO], [MANUAL]

(Factory setting: [AUTO])

### [CH3 LEVEL]

Select auto/manual for the method to adjust the recording level of the audio channel 3.

The items that can be set are as follows.

- [AUTO], [MANUAL]

(Factory setting: [AUTO])

### [CH4 LEVEL]

Select auto/manual for the method to adjust the recording level of the audio channel 4.

The items that can be set are as follows.

- [AUTO], [MANUAL]

(Factory setting: [AUTO])

### [CH1 LEVEL CONTROL]

The recording level can be manually adjusted when [CH1 LEVEL] which adjusts the recording level of the audio channel 1 is set to [MANUAL].

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [70])

### [CH2 LEVEL CONTROL]

The recording level can be manually adjusted when [CH2 LEVEL] which adjusts the recording level of the audio channel 2 is set to [MANUAL].

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [70])

### [CH3 LEVEL CONTROL]

The recording level can be manually adjusted when [CH3 LEVEL] which adjusts the recording level of the audio channel 3 is set to [MANUAL].

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [70])

### [CH4 LEVEL CONTROL]

The recording level can be manually adjusted when [CH4 LEVEL] which adjusts the recording level of the audio channel 4 is set to [MANUAL].

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [70])

### [CH1 MIC LOWCUT]

Enables/disables the lowcut filter for audio channel 1.

The items that can be set are as follows.

- [FRONT], [W.L.], [REAR], [OFF]

(Factory setting: [OFF])

### [CH2 MIC LOWCUT]

Enables/disables the lowcut filter for audio channel 2.

The items that can be set are as follows.

- [FRONT], [W.L.], [REAR], [OFF]

(Factory setting: [OFF])

### [CH3 MIC LOWCUT]

Enables/disables the lowcut filter for audio channel 3.

The items that can be set are as follows.

- [FRONT], [W.L.], [REAR], [OFF]

(Factory setting: [OFF])

### [CH4 MIC LOWCUT]

Enables/disables the lowcut filter for audio channel 4.

The items that can be set are as follows.

- [FRONT], [W.L.], [REAR], [OFF]

(Factory setting: [OFF])

### [CH1 LIMITER]

Enables/disables the limiter when the method to adjust the recording level for audio channel 1 is manual.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [CH2 LIMITER]

Enables/disables the limiter when the method to adjust the recording level for audio channel 2 is manual.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [CH3 LIMITER]

Enables/disables the limiter when the method to adjust the recording level for audio channel 3 is manual.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [CH4 LIMITER]

Enables/disables the limiter when the method to adjust the recording level for audio channel 4 is manual.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [HEAD ROOM]

Sets the headroom (standard level).

The items that can be set are as follows.

- [18dB], [20dB]

(Factory setting: [20dB] (when [AREA SETTINGS] is set to [AREA 1]/[AREA 2]), [18dB] (when [AREA SETTINGS] is set to [AREA 3]/[AREA 4]))

## [OUTPUT SETTINGS]

### [MONITOR SELECT]

Selects the signal format to output to the monitor when the <MONITOR SELECT> switch is set to <ST> (stereo).

The items that can be set are as follows.

- [STEREO], [MIX]

(Factory setting: [STEREO])

### [AUDIO OUT LEVEL]

Selects the audio output level.

The items that can be set are as follows.

- [−3dB], [0dB], [4dB]

(Factory setting: [4dB] (when [AREA SETTINGS] is [AREA 1]/[AREA 2]/[AREA 4]), [0dB] (when [AREA SETTINGS] is [AREA 3]))

### [HDMI OUT CH]

Selects the audio channel to be output from the <HDMI> terminal.

[CH1/2] | Outputs the audio signals of the audio channel 1 and the audio channel 2 as stereo.
[CH3/4] | Outputs the audio signals of the audio channel 3 and the audio channel 4 as stereo.

(Factory setting: [CH1/2])

## [ALARM]

### [BATTERY NEAR END]

Sets whether to sound the alarm when the remaining battery level is near end.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [BATTERY NEAR END CANCEL]

When set to [ON], the output alarm sound or warning displayed for the battery near end can be cancelled by pressing the <MARKER SEL>/<MODE CHECK> switch to the <MCK> side.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [BATTERY END]

Sets whether to sound the alarm when the remaining battery level is exhausted.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [MEDIA NEAR END]

Sets whether to sound the alarm when the remaining memory card capacity is near end.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [MEDIA END]

Sets whether to sound the alarm when the remaining memory card capacity is exhausted.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [WARNING]

Sets whether to sound the alarm when a system error or warning occurs.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

Top of the page