- Top
- Shooting
- Display of the viewfinder status
- Screen display during shooting

# Screen display during shooting

1. Time code/User bits/Counter data

   Displays the time data selected with the <DISPLAY> switch.

   - [TCG :::]: Displays the time code. [TCR :::] will be displayed during playback.

     [TCG] is displayed with black and white inverted during the slave lock into the external input time code.

   - [UBG ]: Displays the user bits. [UBR ] will be displayed during playback.

   - [CLP :::]: Displays the counter value of each clip. This is displayed when the [RECORDING] menu → [REC COUNTER] → [CLIP] is set. Displays the counter value of the clip being played back during playback.

   - [:::]: Displays the cumulative counter value from the reset position. This is displayed when the [RECORDING] menu → [REC COUNTER] → [TOTAL] is set.

2. Bonding Device Status

   Displays the device status received from the bonding device with up to first five letters and the following symbol.

   - : The signal reception strength of the bonding device is displayed in 6 levels.

   - : The remaining battery of the bonding device is displayed in 6 levels.

   - : Displayed when there is an error in the bonding device.

   - (No display): Bonding device is not connected.

3. Recording status

   - [REC]: Recording.

   - [REC] (Flashing): Processing to stop the recording.

   - [P]: Recording is stopped with pre-recording is enabled.

   - (No display): It is in one of the following conditions.

     - Recording is stopped with pre-recording is disabled.

     - It is set to the [NETWORK] menu → [NETWORK FUNC] → [NDI|HX].

4. Recording media

   Setting status of the [RECORDING] menu → [REC MEDIA] is displayed.

   - [eP2]: Displays when set to the [RECORDING] menu → [REC MEDIA] → [expressP2].

   - [mP2]: Displays when set to the [RECORDING] menu → [REC MEDIA] → [microP2/SD].

   - (No display): Set to the [NETWORK] menu → [NETWORK FUNC] → [NDI|HX].

5. Status of the card slot 1 or 2

   Displays status of the card slot 1 when the [RECORDING] menu → [REC MEDIA] → [expressP2] is set.

   Displays status of the card slot 2 when the [RECORDING] menu → [REC MEDIA] → [microP2/SD] is set.

   The status are as follows:

   - : Not target for recording.

   - (flashing): Recognizing the memory card.

   - : Recording target.

   - (No display): It is in one of the following conditions.

     - A memory card has not been inserted.

     - The memory card cannot be recognized.

     - It is set to the [NETWORK] menu → [NETWORK FUNC] → [NDI|HX].

6. Remaining capacity and status of the memory card in card slot 1 or 2

   Displays the remaining capacity and status of the memory card in card slot 1 or 2.

   - [0min]…[999min]: Displays remaining capacity of the memory card. Remaining capacity of 999 minutes or more is displayed as [999min].

     - The display will flash when the remaining capacity of the memory card becomes two minutes or less.

     - The remaining capacity of the memory card available for simultaneous recording (remaining capacity for the memory card of the two memory cards with less remaining capacity) is displayed when simultaneous recording is performed.

   - [WP]: It is write protected. The write-protected switch on the memory card is set to the Protect side or the LOCK side.

   - [END]: Memory card has no remaining capacity.

   - [ERR]: Memory card that cannot record is inserted. Displayed when the card is recognized but cannot be used, such as having a format error, or not being a memory card.

   - [!SDXC]: Recording format is set to MOV but SDXC memory card, expressP2 card, or 64 GB microP2 card is not inserted.

   - (No display): It is in one of the following conditions.

     - A memory card has not been inserted.

     - The memory card cannot be recognized.

     - It is set to the [NETWORK] menu → [NETWORK FUNC] → [NDI|HX].

7. Message display area for wireless audio warning and cooling fan stop

   Displays a warning when the wireless audio reception status becomes poor.

   Displays a message when the cooling fan has stopped.

8. SDI/HDMI remote control status

   Displays the control status of the recording start and recording stop on the external equipment connected to the <SDI OUT1>/<SDI OUT2>/<HDMI> terminals.

   - [REC S/H]: Recording instruction is output to the output from the <SDI OUT1>/<SDI OUT2>/<HDMI> terminals.

   - [S/H]: Pause instruction is output to the output from the <SDI OUT1>/<SDI OUT2>/<HDMI> terminals.

   - [REC SDI]: Recording instruction is output to the output from the <SDI OUT1>/<SDI OUT2> terminals.

   - [SDI]: Pause instruction is output to the output from the <SDI OUT1>/<SDI OUT2> terminals.

   - [REC HDMI]: Recording instruction is output to the output from the <HDMI> terminal.

   - [HDMI]: Pause instruction is output to the output from the <HDMI> terminal.

9. Status of card slot 3

   It is not displayed when set to the [RECORDING] menu → [REC MEDIA] → [expressP2].

   - : Not target for recording.

   - (flashing): Recognizing the memory card.

   - : Recording target.

   - (No display): It is in one of the following conditions.

     - A memory card has not been inserted.

     - The memory card cannot be recognized.

     - The [NETWORK] menu → [NETWORK FUNC] → [NDI|HX] is set.

10. Remaining capacity and status of the memory card in card slot 3

    Displays the remaining capacity and status of the memory card in card slot 3.

    It is not displayed when set to the [RECORDING] menu → [REC MEDIA] → [expressP2].

    - [0min]…[999min]: Displays remaining capacity of the memory card. Remaining capacity of 999 minutes or more is displayed as [999min].

      - The display will flash when the remaining capacity of the memory card becomes two minutes or less.

      - The remaining capacity of the memory card available for simultaneous recording (remaining capacity for the memory card of the two memory cards with less remaining capacity) is displayed when simultaneous recording is performed.

    - [WP]: It is write protected. The write-protected switch of the memory card is set to the LOCK side.

    - [END]: Memory card has no remaining capacity.

    - [ERR]: Memory card that cannot record is inserted. Displayed when the card is recognized but cannot be used, such as having a format error, or not being a memory card.

    - [!SDXC]: Recording format is set to MOV but SDXC memory card or 64 GB microP2 card is not inserted.

    - (No display): It is in one of the following conditions.

      - A memory card has not been inserted.

      - The memory card cannot be recognized.

      - It is set to the [NETWORK] menu → [NETWORK FUNC] → [NDI|HX].

11. Special recording function

    Displays the status of special recording function.

    - [INTRVL]: Interval recording is enabled.

    - [I-REC]: During interval recording or recording is paused.

    - (No display): It is in one of the following conditions.

      - Interval recording is disabled.

      - It is set to the [NETWORK] menu → [NETWORK FUNC] → [NDI|HX].

12. Two-slot function

    Displays the setting status of the recording function using two card slots.

    It is displayed with a slanted line if it is in a condition that cannot perform two-slot function even if each function is enabled.

    - [RELAY]: Relay recording is enabled.

    - [SIMUL]: Simultaneous recording is enabled.

    - [NDI|HX]: It is set to the [NETWORK] menu → [NETWORK FUNC] → [NDI|HX].

    - (No display): In standard recording status.

13. Flash band compensation function

    - [FBC]: Flash band compensation function is enabled.

14. Streaming status

    Displays the streaming status.

    - : The camera is connected to a device to receive the streaming video, and the streaming video is distributed.

    - (flashing): When the camera is trying to connect to a device to receive the streaming video

    - : Streaming video is not being streamed.

    - : There is an error in the streaming function and cannot operate.

    - (No display): Streaming function is disabled

15. High dynamic range function/dynamic range stretcher function

    - [HDR]: It is set to the [SCENE FILE] menu → [GAMMA MODE SEL] → [HLG].

    - [DRS]: Dynamic range stretcher function is enabled.

16. Connection status of the wireless LAN/wired LAN

    Displays the connection status of the wireless LAN or wired LAN.

    - : Set to wireless LAN and not connected to the ROP app.

    - : Set to wireless LAN and connected to the ROP app.

    - : Set to wireless LAN but the wireless LAN is not operating properly.

    - : Set to wired LAN and not connected to the ROP app.

    - : Set to wired LAN and connected to the ROP app.

    - : Set to wired LAN but the wired LAN is not operating properly.

    - (No display): Both the wireless LAN and the wired LAN are disabled.

17. Remaining battery level

    - [.V]: Displays the charge level of batteries with no charge level information in 0.1 V units. The display will flash when the remaining charge is at the near end setting value or below.

    - [%]: Displays the charge level of batteries with charge level information in %. The display will flash when the remaining charge is at the near end setting value or below.

    - [EMP]: Displayed when there is no charge level on batteries with charge level information or the level is at the near end setting value or below.

    - [MAX]: Displayed when batteries with charge level information are fully charged.

18. Chromatic aberration compensation function

    - [CAC]: Chromatic aberration compensation function is enabled.

19. Gamma mode

    Setting value for the gamma mode selected in the [SCENE FILE] menu → [GAMMA MODE SEL] is displayed.

    - [HD]

    - [SD]

    - [FLK1]

    - [FLK2]

    - [FLK3]

    - [FREC]

    - [VREC]

    - [HLG]

20. Scene file name

    Name of the scene file selected in the [SCENE FILE] menu → [FILE SELECT] is displayed.

21. Waveform monitor

    Displays the video status in waveform or vector.

    Displayed only on the LCD monitor and the viewfinder.

22. Type of marker

    Displays the type of currently displayed marker in the STATUS screen of the mode check.

    [MKR:A]: Displays the marker type [A].

    [MKR:B]: Displays the marker type [B].

    [MKR:OFF]: Marker is not displayed.

23. Digital zoom

    Displays the digital zoom ratio.

    - [D2×]: Two times

    - [D3×]: Three times

    - [D4×]: Four times

24. Focus

    Displays the focus value.

    The display of the focus value follows the setting in the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [ZOOM/FOCUS].

    - [MF]: Displays in the position value from [00] to [99] when set to the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [ZOOM/FOCUS] → [NUMBER].

    - [MFft]: Displays in feet unit when set to the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [ZOOM/FOCUS] → [mm/feet].

    - [MFm]: Displays in meter unit when set to the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [ZOOM/FOCUS] → [mm/m].

    - (No display): Focus value cannot be acquired.

25. Zoom

    Displays the zoom value.

    The display of the zoom value follows the setting in the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [ZOOM/FOCUS].

    - [Z]: Displays in the position value from [000] to [999] when set to the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [ZOOM/FOCUS] → [NUMBER].

    - [Z.]: Displays in millimeter unit when set to the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [ZOOM/FOCUS] → [mm/feet] or [mm/m].

    - (No display): Zoom value cannot be acquired.

26. Super black

    - [B]: Displayed when the super black function is enabled.

27. Iris

    Displays the F value.

    Displayed when a lens with an F value display function is used.

    Flashes when changing the setting value of the iris override function.

    - [F]: Displays the F value of the lens.

    - [OPEN]: Displayed when the lens aperture is open.

    - [CLOSE]: Displayed when the lens aperture is closed.

    - [NC]: Displayed when the lens cable is not connected.

28. Super iris

    - [S]: Displayed when the super iris function is enabled.

29. High-sensitivity mode

    - [H.SENS.]: Displayed when set to the [SYSTEM] menu → [SHOOTING MODE] → [HIGH SENS.].

30. Iris override

    Displays the compensation level when the iris override function is enabled.

    Flashes when changing the compensation level.

    - [+]: Aperture opens by about 0.5.

    - [++]: Aperture opens by about 1.

    - [−]: Aperture closes by about 0.5.

    - [−−]: Aperture closes by about 1.

    - (No display): It is in one of the following conditions.

      - Iris is a reference value.

      - Iris override function is disabled.

31. Luminance drop message display

    Displayed when luminance has dropped.

32. Luminance of Y GET

    Displays the luminance level when the Y GET function is enabled.

33. Shutter speed

    - [1/]: Displays the shutter speed.

    - [1/]: Displays the shutter speed in time (minutes) when synchro scan function is enable and the [SCENE FILE] menu → [SYNC SCAN TYPE] → [sec] is set.

    - [d]: Displays the shutter speed in open angle when synchro scan function is enable and the [SCENE FILE] menu → [SYNC SCAN TYPE] → [deg] is set.

    - [HALF]: Displays when the [CAMERA] menu → [SHUTTER SPEED] → [POSITION1] to [POSITION6] → [HALF] is set and the position is selected.

    - (No display): Electronic shutter function is disabled.

34. Date and time information

    Displays the date and time information.

    The display contents follow the setting in the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [DATE/TIME]. ([DATE/TIME])

    The display order for the year, month, and date follows the setting in the [OTHERS] menu → [CLOCK] → [DATE FORMAT].

    - [Y-M-D]: Displays in yyyy mmm dd hh:mm:ss format.

    - [M-D-Y]: Displays in mmm dd yyyy hh:mm:ss format.

    - [D-M-Y]: Displays in dd mmm yyyy hh:mm:ss format.

      - mmm: Month (JAN (January), FEB (February), MAR (March), APR (April), MAY (May), JUN (June), JUL (July), AUG (August), SEP (September), OCT (October), NOV (November), DEC (December))

      - dd: Date

      - yyyy: Year

      - hh: Hour

      - mm: Minute

      - ss: Second

35. Digital super gain

    Displays the digital super gain value when the digital super gain function is enabled.

36. Gain

    Displays the gain value.

    - [dB]: Displays the current gain value.

    - [AGC]: Displayed when the auto gain control is enabled.

37. Auto knee

    - [AUTO KNEE:ON]: Auto knee function is enabled.

    - [AUTO KNEE:OFF]: Auto knee function is disabled.

38. Color temperature

    Displays the position and color temperature selected with the <WHITE BAL> switch.

    - [ATW]: Displayed when the auto tracking white balance is operating.

    - [LOCK]: Displayed when the auto tracking white balance is locked.

    - [AK]: The <WHITE BAL> switch is set to memory <A>.

    - [BK]: The <WHITE BAL> switch is set to memory <B>.

    - [PK]: The <WHITE BAL> switch is set to <PRST>.

39. Audio level meter

    Displays the status of audio input setting and recording level.

    Audio channel to display can be changed using the audio channel selector switch.

    - [1: 2:]: Displayed when the audio channel selector switch is set to <CH1/2>.

      Audio input setting for audio channel 1 and audio channel 2 are displayed in .

      F is displayed when the <AUDIO IN CH1>/<AUDIO IN CH2> switch is set to <FRONT>. W is displayed when the <AUDIO IN CH1>/<AUDIO IN CH2> switch is set to <W.L.>. R is displayed when the <AUDIO IN CH1>/<AUDIO IN CH2> switch is set to <REAR>.

    - [3: 4:]: Displayed when the audio channel selector switch is set to <CH3/4>.

      Audio input setting for audio channel 3 and audio channel 4 are displayed in .

      F is displayed when the <AUDIO IN CH3>/<AUDIO IN CH4> switch is set to <FRONT>. W is displayed when the <AUDIO IN CH3>/<AUDIO IN CH4> switch is set to <W.L.>. R is displayed when the <AUDIO IN CH3>/<AUDIO IN CH4> switch is set to <REAR>.

    A white frame is displayed at the position of the reference level set in the [AUDIO] menu → [REC CH SETTINGS] → [HEAD ROOM]. (Eighth from the left when set to [20dB], ninth from the left when set to [18dB])

    - : Displayed when audio cannot be recorded.

40. Filter position

    Displays the <ND FILTER> dial position with numbers 1 to 4 and <CC FILTER> dial position with alphabet A to D.

    [-] will flash by inverting black and white when the filter position is not set correctly.

41. Extender

    - [EX]: Displayed when the lens extender function is functioning.

42. Remote control status in an IP connection

    - [IP REMOTE]: Displayed when the remote control is possible in the IP connection.

    - [IP REMOTE] (flashing): Displayed when waiting for the connection in the IP connection.

    - (No display): Remote control function in an IP connection is disabled.

43. Error display of auto black balance

    Displays the status when the adjustment result of the auto black balance was abnormal.

44. Error display of auto white balance

    Displays the status when the adjustment result of the auto white balance was abnormal.

45. Message display area

    Displayed when there is a message or warning about the camera status.

46. Message for invalid filter position

    Message is displayed when power is turned on if the <ND FILTER>/<CC FILTER> dial is not set correctly.

    Message is displayed when performing the auto white balance if the <CC FILTER> dial is not set correctly.

47. Clip name

    Displays the name of the clip being recorded with up to eight characters from the start.

48. Recording format

    Displays the file format set in the [SYSTEM] menu → [FILE FORMAT] and the recording codec set in the [SYSTEM] menu → [REC FORMAT].

    It is not displayed when set to the [NETWORK] menu → [NETWORK FUNC] → [NDI|HX].

    - [P2 AVC-I422]

    - [P2 AVC-G50]

    - [P2 AVC-G25]

    - [P2 AVC-G12]

    - [MOV 420 150M]

    - [MOV 420 100M]

    - [MOV 422 150M]

    - [MOV 422 100M]

    - [MOV 422 50M]

    - [MOV HEVC 200M]

    - [MOV HEVC 150M]

    - [MOV HEVC 100M]

    - [MOV ALL-I 400M]

    - [MOV ALL-I 200M]

    - [MOV ALL-I 100M]

49. System resolution/system frequency

    Displays the system resolution and the system frequency set in the [SYSTEM] menu → [REC FORMAT].

    - [2160-59.94p]

    - [2160-50.00p]

    - [2160-29.97p]

    - [2160-25.00p]

    - [2160-23.98p]

    - [1080-59.94p]

    - [1080-50.00p]

    - [1080-29.97p]

    - [1080-25.00p]

    - [1080-23.98p]

    - [1080-59.94i]

    - [1080-50.00i]

    - [720-59.94p]

    - [720-50.00p]

Top of the page