- Top
- Operation
- Menu settings
- [CAMERA] menu

# [CAMERA] menu

Sets the basic camera function.

This menu cannot be set when the thumbnail screen is displayed.

## [SHUTTER SPEED]

The items that can be set in [POSITION1] to [POSITION6] are as follows.

- When the [SYSTEM] menu → [FREQUENCY] → [59.94Hz] is set

  - [OFF], [1/100], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF]

- When the [SYSTEM] menu → [FREQUENCY] → [50.00Hz] is set

  - [OFF], [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF]

[SYNCHRO SCAN] | [SYNCHRO SCAN] is assigned as the shutter speed selected by the <SHUTTER> switch. The items that can be set are as follows. [ON], [OFF] (Factory setting: [ON])
[POSITION1] | Sets the shutter speed of [POSITION1]. The factory setting varies depending on the [SYSTEM] menu → [FREQUENCY] setting. (Factory setting: [1/100] (when [59.94Hz] is set), [1/60] (when [50.00Hz] is set))
[POSITION2] | Sets the shutter speed of [POSITION2]. (Factory setting: [1/120])
[POSITION3] | Sets the shutter speed of [POSITION3]. (Factory setting: [1/250])
[POSITION4] | Sets the shutter speed of [POSITION4]. (Factory setting: [1/500])
[POSITION5] | Sets the shutter speed of [POSITION5]. (Factory setting: [1/1000])
[POSITION6] | Sets the shutter speed of [POSITION6]. (Factory setting: [1/2000])

## [SW MODE]

### [RET SW]

Sets the function when the <RET> button on the lens is pressed.

[INHIBIT] | Does not assign a function.
[D.ZOOM] | Assigns the digital zoom function. Zooms in on the field angle by 2x, 3x and 4x vertically and horizontally.
[FOCUS ASSIST] | Displays/hides the focus assist display. Select the type of display in the [VIDEO OUT/LCD/VF] menu → [FOCUS ASSIST] → [FOCUS ASSIST SELECT].
[REC CHECK] | Automatically plays back the last approximately three seconds of the previously shot clip.
[LCD/VF DETAIL] | Emphasizes the contour of the image in the viewfinder or LCD monitor to make it easier to focus.
[VF COLOR] | Selects whether to display viewfinder images in color or in black and white. This is interlocked with the setting value in the [VIDEO OUT/LCD/VF] menu → [VF COLOR].
[STREAMING START] | Assigns the function for starting or stopping streaming from the camera. This is interlocked with the setting value in the [NETWORK] menu → [STREAMING] → [START].

(Factory setting: [REC CHECK])

### [S.BLK LEVEL]

Sets the super black level.

The items that can be set are as follows.

- [−30], [−20], [−10]

(Factory setting: [−10])

### [AUTO KNEE SW]

Enables/disables the auto knee function and the dynamic range stretcher function.

[DRS] | The dynamic range stretcher function is enabled when the <OUTPUT>/<AUTO KNEE> switch is set to <ON>.
[ON] | The auto knee function is enabled when the <OUTPUT>/<AUTO KNEE> switch is set to <ON>.
[OFF] | The auto knee function and the dynamic range stretcher function are not enabled even if the <OUTPUT>/<AUTO KNEE> switch is set to <ON>.

(Factory setting: [ON])

### [SHD,ABB SW CTL]

Sets whether to automatically adjust black shading when the <AUTO W/B BAL> switch is pressed toward <ABB> side for two seconds or more.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [S.GAIN OFF]

Selects a method to release super gain mode.

[L/M/H] | The super gain mode is released in following cases. When the <GAIN> switch setting is changed When the USER button assigned with [S.GAIN] is pressed
[S.GAIN] | The super gain mode is released only when the USER button assigned with [S.GAIN] is pressed.

(Factory setting: [L/M/H])

### [DS.GAIN OFF]

Selects a method to release digital super gain mode (accumulated gain).

[L/M/H] | The digital super gain mode is released in following cases. When the <GAIN> switch setting is changed When the USER button assigned with [DS.GAIN] is pressed
[DS.GAIN] | The digital super gain mode is released only when the USER button assigned with [DS.GAIN] is pressed.

(Factory setting: [DS.GAIN])

### [D.ZOOM]

Selects the zoom ratio for when the USER button assigned with [D.ZOOM] is pressed.

The items that can be set are as follows.

- [×2], [×3], [×4], [ALL]

(Factory setting: [ALL])

## [USER SW]

The function to be assign to the USER button can be set.

Following functions can be assigned.

- [INHIBIT], [DRS], [FBC], [S.GAIN], [ATW], [ATW LOCK], [Y GET], [D.ZOOM], [DS.GAIN], [S.IRIS], [I.OVR], [S.BLK], [B.GAMMA], [FOCUS ASSIST], [C.TEMP], [PRE REC], [REC CHECK], [DEL LAST CLIP], [SLOT SEL], [REC SW], [WFM], [LCD/VF HDR], [LCD/VF DETAIL], [VF COLOR], [INDICATOR SW], [LOAD SETUP FILE], [LCD BACKLIGHT], [CARD READER MODE], [STREAMING START]

For details, refer to “Assigning function to the USER buttons”.

[USER1] | Sets the function to assign to the <USER 1> button. (Factory setting: [FOCUS ASSIST])
[USER2] | Sets the function to assign to the <USER 2> button. (Factory setting: [S.GAIN])
[USER3] | Sets the function to assign to the <USER 3> button. (Factory setting: [DS.GAIN])
[USER4] | Sets the function to assign to the <USER 4> button. (Factory setting: [Y GET])
[USER5] | Sets the function to assign to the <USER 5> button. (Factory setting: [WFM])

## [WHITE BALANCE MODE]

### [FILTER INH]

Selects whether to hold or not hold the white balance memory (Ach and Bch) data for each CC filter.

[ON] | Holds Ach and Bch memory data (two memories), regardless of the CC filter.
[OFF] | Holds Ach and Bch memory data (eight memories), for each CC filter.

(Factory setting: [ON])

### [SHOCKLESS AWB]

When the position of the <WHITE BAL> switch is changed, set the time until it transfers to the white balance condition at the changed position.

[FAST] | Transfers to the white balance condition in approximately one second.
[NORMAL] | Transfers to the white balance condition in approximately two seconds.
[SLOW1] | Transfers to the white balance condition in approximately three seconds.
[SLOW2] | Transfers to the white balance condition in approximately ten seconds.
[SLOW3] | Transfers to the white balance condition in approximately 20 seconds.
[OFF] | Transfers immediately.

(Factory setting: [NORMAL])

### [AWB AREA]

Selects the detection area to perform the auto adjustment of the white balance.

[25%] | Detects 25% of the area near screen center.
[50%] | Detects 50% of the area near screen center.
[90%] | Detects 90% of the screen area.

(Factory setting: [25%])

### [ATW]

Assigns the setting of the auto tracking white balance function to the <WHITE BAL> switch.

The items that can be set are as follows.

- [Ach], [Bch], [PRE], [OFF]

(Factory setting: [OFF])

### [ATW SPEED]

Sets the control speed of the auto tracking white balance function.

The items that can be set are as follows.

- [FAST], [NORMAL], [SLOW]

(Factory setting: [NORMAL])

### [ATW TARGET R]

Finely adjusts the Rch output for convergence with the auto tracking white balance operation.

The items that can be set are as follows.

- [−10]…[+10]

(Factory setting: [0])

### [ATW TARGET B]

Finely adjusts the Bch output for convergence with the auto tracking white balance operation.

The items that can be set are as follows.

- [−10]…[+10]

(Factory setting: [0])

### [W.BAL PRESET]

Sets the color temperature to be assigned to <PRST> of the <WHITE BAL> switch.

The items that can be set are as follows.

- [3200K], [5600K], [VAR]

(Factory setting: [3200K])

### [W.BAL VAR]

Sets the value of [VAR] in [W.BAL PRESET].

Enabled when [W.BAL PRESET] is set to [VAR] and the <WHITE BAL> switch is at <PRST>.

The items that can be set are as follows.

- When the <CC FILTER> dial is set to <A>

  - [2000K]…[15000K]

- When the <CC FILTER> dial is set to <B>

  - [2380K]…[>15000K]

- When the <CC FILTER> dial is set to <C>

  - [2730K]…[>15000K]

- When the <CC FILTER> dial is set to <D>

  - [2890K]…[>15000K]

(Factory setting: [3200K])

## [USER SW GAIN]

### [S.GAIN]

Selects the super gain value to enable when [S.GAIN] is assigned to the USER button.

- When set to [ALL], the display will switch in the order of [30dB], [36dB], [42dB], and normal gain every time the USER button is pressed.

The items that can be set are as follows.

- [30dB], [36dB], [42dB], [ALL]

(Factory setting: [ALL])

### [DS.GAIN]

Selects the digital super gain value to enable when [DS.GAIN] is assigned to the USER button.

- When set to [ALL], the display will switch in the order of [6dB], [10dB], [12dB], [15dB], [20dB], [24dB], [28dB], [34dB], and normal gain every time the USER button is pressed.

The items that can be set are as follows.

- [6dB], [10dB], [12dB], [15dB], [20dB], [24dB], [28dB], [34dB], [ALL]

(Factory setting: [ALL])

## [LENS/IRIS]

### [A.IRIS LEVEL]

Sets the auto iris target value.

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [50])

### [A.IRIS PEAK/AVE]

Sets the ratio included in the peak for auto iris standard.

Larger the ratio, it will correspond to a peak within the iris detection window.

Smaller the ratio, it will correspond to a average value within the iris detection window.

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [30])

### [A.IRIS WINDOW]

Selects the auto iris detection window.

[NORMAL1] | Window that is around center of the screen.
[NORMAL2] | Window that is around bottom of the screen.
[CENTER] | Window that is a spot around center of the screen.

(Factory setting: [NORMAL1])

### [S.IRIS LEVEL]

Sets the super iris (backlight compensation) target value.

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [70])

### [IRIS GAIN]

Sets whether to perform the [IRIS GAIN] adjustment on the camera or on the lens.

The items that can be set are as follows.

- [CAM], [LENS]

(Factory setting: [LENS])

### [IRIS GAIN VALUE]

Selects the [IRIS GAIN] adjustment value.

This setting is enabled when [IRIS GAIN] is set to [CAM].

The items that can be set are as follows.

- [0]…[20]

(Factory setting: [10])

## [LENS ADJ.]

### [F2.8 ADJ.]

Iris is set to F2.8 only when set to [ON].

(Adjusts the iris so that it becomes F2.8 at the lens side)

When moved from the [F2.8 ADJ.] setting screen, it is forcefully switched to [OFF].

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

### [F16 ADJ.]

Iris is set to F16 only when set to [ON].

(Adjusts the iris so that it becomes F16 at the lens side)

When moved from the [F16 ADJ.] setting screen, it is forcefully switched to [OFF].

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [OFF])

## [LENS FILE ADJ.]

NOTE

- Data adjusted with [LENS FILE ADJ.] can be saved as a lens file to the SD card.

### [LENS FILE ADJ. MODE]

Selects the mode to adjust the lens.

When transferred from the [LENS FILE ADJ. MODE] setting screen, it is forcefully switched to [OFF].

[ON] | The gains of Rch and Bch adjusted in the [SCENE FILE] menu → [RB GAIN CONTROL SETTING] and the flare level of Rch, Gch, and Bch adjusted in the [SCENE FILE] menu → [RGB BLACK CONTROL SETTING] are disabled.
[OFF] | The gains of Rch and Bch adjusted in the [SCENE FILE] menu → [RB GAIN CONTROL SETTING] and the flare level of Rch, Gch, and Bch adjusted in the [SCENE FILE] menu → [RGB BLACK CONTROL SETTING] are enabled.

(Factory setting: [OFF])

### [LENS R GAIN OFFSET]

Corrects the Rch sensitivity of the lens to use.

The items that can be set are as follows.

- [−200]…[200]

(Factory setting: [0])

### [LENS B GAIN OFFSET]

Corrects the Bch sensitivity of the lens to use.

The items that can be set are as follows.

- [−200]…[200]

(Factory setting: [0])

### [LENS R FLARE]

Adjusts the Rch flare level.

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [0])

### [LENS G FLARE]

Adjusts the Gch flare level.

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [0])

### [LENS B FLARE]

Adjusts the Bch flare level.

The items that can be set are as follows.

- [0]…[100]

(Factory setting: [0])

## [AGC]

Sets the operation of the auto gain control.

[ON] | Performs the operation of the [AGC] function that automatically adjusts camera gain.
[OFF] | Does not perform the operation of the [AGC] function that automatically adjusts camera gain.

(Factory setting: [OFF])

### [AGC LIMIT]

Sets the maximum gain value during [AGC] operation.

The items that can be set are as follows.

- [3dB], [6dB], [12dB], [18dB]

(Factory setting: [6dB])

### [AGC POINT]

Sets the F value to switch control from auto iris to [AGC] during [AGC] operation.

The items that can be set are as follows.

- [F2.8], [F4.0], [F5.6]

(Factory setting: [F4.0])

## [BLACK SHADING]

### [CORRECT]

Enables/disables the black shading correction.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [DETECTION]

Executes the black shading correction.

## [WHITE SHADING]

[CORRECT] | Enables/disables the white shading correction. The items that can be set are as follows. [ON], [OFF] (Factory setting: [ON])
[R H SAW] | Performs the white shading correction manually. Adjusts sawtooth waveforms and parabolic waveforms of RGB channels in the horizontal and vertical directions. The items that can be set are as follows. [−255]…[255] (Factory setting: [0])
[R H PARA]
[R V SAW]
[R V PARA]
[G H SAW]
[G H PARA]
[G V SAW]
[G V PARA]
[B H SAW]
[B H PARA]
[B V SAW]
[B V PARA]

## [CAC ADJ.]

### [CAC CONTROL]

Switches [ON]/[OFF] of the chromatic aberration compensation (CAC).

[ON] | Performs the chromatic aberration compensation.
[OFF] | Does not perform the chromatic aberration compensation.

(Factory setting: [ON])

### [LIST/DELETE]

Views the list of CAC file stored in the camera memory or deletes the file with the number selected from the list of the CAC file.

The items that can be selected are as follows.

- [No1]…[No32]

Top of the page