- Top
- Shooting
- Special recording function
- Recording check function

# Recording check function

- After recording ends, pressing the <RET> button on the lens automatically plays back the last few seconds of the latest clip.

  Check whether video has been recorded properly. After playback, the camera is again ready to start recording.

- The recording check function can be assigned to a USER button. Set in the [CAMERA] menu → [USER SW] → [USER1] to [USER5] → [REC CHECK].

REC check will not operate in following cases.

- When the power is turned on/off

- When restarted

- When the <THUMBNAIL> button is pressed

- When the memory card is inserted/ejected

- When formatted the memory card

- When the recording target card slot is switched by pressing the USER button assigned with [SLOT SEL]

- When switched to [CARD READER MODE]

- When set to the [RECORDING] menu → [2 SLOTS FUNC.] → [SIMUL REC]

- When either of the following settings are changed

  - [SYSTEM] menu → [FILE FORMAT]

  - [SYSTEM] menu → [REC FORMAT]

  - [RECORDING] menu → [2 SLOTS FUNC.]

NOTE

- Set to the [CAMERA] menu → [SW MODE] → [RET SW] → [REC CHECK].

- During recording check, playback image is output not only to the viewfinder but also to the video output terminals (<SDI OUT1> terminal, <SDI OUT2> terminal, and <HDMI> terminal). Note that, when a backup device is connected and a backup image is being recorded, the playback image currently under recording check will be recorded.

Top of the page