- Top
- Operation
- Basic operation of the menu
- Basic operation of the menu

# Basic operation of the menu

The setting of the camera can be changed with the menu in accordance to the shooting scene or recording contents.

Set data is written and saved in the camera memory.

Various settings are possible from the menu.

There are two methods of operation, a method to operate with the jog dial button or the cursor operation button, and a method to touch the LCD monitor.

## When operating with the button

Operate by turning or pressing the jog dial button on the camera.

It can also be operated by pressing the cursor operation button and the <SET> button.

[MENU]>[CAMERA]>[LENS/IRIS]>[A.IRIS LEVEL]

[EXIT]

[EXIT]

[CAMERA]

[EXIT]

[SCENE FILE]

[SHUTTER SPEED]

[SYNCHRO SCAN]

[ON]

[ON]

[AUDIO]

[SW MODE]

[POSITION1]

[1/100]

[OFF]

[VIDEO OUT/LCD/VF]

[USER SW]

[POSITION2]

[1/120]

[RECORDING]

[WHITE BALANCE MODE]

[POSITION3]

[1/250]

[NETWORK]

[USER SW GAIN]

[POSITION4]

[1/500]

[LENS/IRIS]

[SYSTEM]

[1/1000]

[POSITION5]

[OTHERS]

[LENS ADJ.]

[POSITION6]

[1/2000]

Fig. 1

Fig. 2

Press the <MENU> button when not recording.

The menu is displayed.

Select the menu to set.

Turn the jog dial button to move the cursor to the item to set.

The cursor can also be moved by pressing the cursor operation button.

Press the jog dial button or the <SET> button.

The lower level menu is displayed.

- The confirmation screen is displayed depending on the menu.

- Perform the similar operation if there is next level.

- In some menus, a screen to set the numeric value is displayed in the camera image. (Fig. 2)

- In some menus, a message is displayed if a menu cannot be executed.

- To return to one level higher, perform the following operation.

  - Press the <EXIT> button.

  - Press the cursor operation button.

  - Place the cursor on [EXIT] at the top and press the <SET> button or the jog dial button.

Select the item to set.

Turn the jog dial button to move the cursor to the item to set.

The cursor can also be moved by pressing the cursor operation button.

Press the jog dial button or the <SET> button.

A check mark is displayed at the left of the set item. (Fig. 1)

- To return to one level higher, perform the following operation.

  - Press the <EXIT> button.

  - Press the cursor operation button.

  - Place the cursor on [EXIT] at the top and press the <SET> button or the jog dial button.

Press the <MENU> button to close the menu.

- Depending on the operating item, it will automatically return to the previous screen.

NOTE

- In the screen to set the numeric value (Fig. 2), the value is changed fast by turning the jog dial button in the direction to change with the button pressed and fixing it or press and hold the cursor operation button.

## When operating by touching the LCD monitor

Operate by touching the LCD monitor.

[CAMERA]

[SCENE FILE]

[AUDIO]

[VIDEO OUT/LCD/VF]

[RECORDING]

[NETWORK]

[SYSTEM]

[OTHERS]

Press the <MENU> button when not recording.

The menu is displayed.

Select the menu to set.

- Touch the menu to set. The lower level menu is displayed.

- The confirmation screen is displayed depending on the menu.

- Perform the similar operation if there is next level.

- In some menus, a screen to set the numeric value is displayed in the camera image.

  To change the numeric value, touch []/[] and change the setting value.

- In some menus, a message is displayed if a menu cannot be executed.

- Touch []/[] to toggle the pages.

  The button icons cannot be touched if there are no more pages.

- To return to one level higher, touch .

Select the item to set.

- Touch the item to set. A check mark is displayed at the left of the set item.

- To return to one level higher, touch .

Exit from the menu by touching , or pressing the <MENU> button.

- Depending on the operating item, it will automatically return to the previous screen.

Top of the page