- Top
- Preparation
- Memory cards
- Preventing accidental erasure

# Preventing accidental erasure

To prevent inadvertently erase the recording contents on the memory card, set the write-protected switch on the memory card to the Protect side or the LOCK side.

Write-protected switch

Write-protected switch

NOTE

- Set the write-protected switch before inserting the card. This will not operated when the write-protected switch is toggled after inserting the card.

Top of the page