- Top
- Description of Parts
- Audio (input) function section

# Audio (input) function section

1. <F.AUDIO LEVEL> dial

   Adjusts the recording level of the audio channel selected in the [AUDIO] menu → [REC CH SETTINGS] → [VOL. SELECT] when the <AUDIO SELECT CH1/3>/<AUDIO SELECT CH2/4> switch is set to <MANU>.

   - Set whether to enable the <F.AUDIO LEVEL> dial at the [AUDIO] menu → [REC CH SETTINGS] → [FRONT VOL. CH1] to [FRONT VOL. CH4].

2. <AUDIO LEVEL CH1/3>/<AUDIO LEVEL CH2/4> dial

   Adjusts the recording level of the audio channel when the <AUDIO SELECT CH1/3>/<AUDIO SELECT CH2/4> switch is set to <MANU>.

   <AUDIO LEVEL CH1/3> dial: Adjusts the recording level of the audio channel 1 or the audio channel 3.

   <AUDIO LEVEL CH2/4> dial: Adjusts the recording level of the audio channel 2 or the audio channel 4.

   - Select the audio channel to adjust with the dial in the [AUDIO] menu → [REC CH SETTINGS] → [VOL. SELECT].

   - Dial is equipped with a lock mechanism. Adjust by turning the dial while pressing it in.

3. <AUDIO IN CH1>/<AUDIO IN CH2>/<AUDIO IN CH3>/<AUDIO IN CH4> switch

   Selects the audio signal to input to the audio channel 1 to audio channel 4.

   <FRONT>: Inputs the audio signal of the microphone connected to the <MIC IN> terminal.

   <W.L.>: Inputs the audio signal from the wireless microphone receiver.

   <REAR>: Inputs the audio signal from the audio device connected to the <AUDIO IN CH1/3> terminal or the <AUDIO IN CH2/4> terminal.

   NOTE

   - When the stereo microphone AJ-MC900G (optional) is used, set both <AUDIO IN CH1> and <AUDIO IN CH2> (or <AUDIO IN CH3> and <AUDIO IN CH4>) to <FRONT>.

     L CH is recorded to the audio channel 1 or the audio channel 3, and R CH is recorded to the audio channel 2 or the audio channel 4, respectively.

4. <AUDIO SELECT CH1/3>/<AUDIO SELECT CH2/4> switch

   Select the audio channel to adjust in the [AUDIO] menu → [REC CH SETTINGS] → [VOL. SELECT].

   <AUDIO SELECT CH1/3> switch: Switches the method to adjust the recording level for the audio channel 1 or audio channel 3 with <AUTO>/<MANU> (automatic/manual).

   <AUDIO SELECT CH2/4> switch: Switches the method to adjust the recording level for the audio channel 2 or audio channel 4 with <AUTO>/<MANU> (automatic/manual).

5. Wireless microphone slot

   Mount the UniSlot wireless microphone receiver (optional).

6. <LINE>/<MIC> selector switch

   Switches the audio signal input from the <AUDIO IN CH1/3>/<AUDIO IN CH2/4> terminal.

   <LINE>: Inputs audio signals from line-input audio equipment.

   <MIC>: Inputs audio signals from the microphone.

7. Microphone input power selector switch

   Turns on/off the power supply to the microphone connected to the <AUDIO IN CH1/3>/<AUDIO IN CH2/4> terminal.

   <+48V>: Supplies +48 V power to the microphone.

   <OFF>: Does not supply power to the microphone.

   NOTE

   - When microphone input <+48V> is set and microphones are not connected to the <AUDIO IN CH1/3> and <AUDIO IN CH2/4> terminals, low-frequency noise may occur. This is not a problem when a microphone is connected.

   - When the [AUDIO] menu → [INPUT SETTINGS] → [REAR MIC POWER] → [ON] is not set, power is not supplied regardless of the switch position.

8. <AUDIO IN CH1/3>/<AUDIO IN CH2/4> terminal

   Connects the audio equipment or the microphone.

   <AUDIO IN CH1/3> terminal: Inputs the audio signal to the audio channel 1 and the audio channel 3.

   <AUDIO IN CH2/4> terminal: Inputs the audio signal to the audio channel 2 and the audio channel 4.

9. Cable holder

   Fixes HDMI cables, etc.

10. Cable holder

    Fixes the cables for lights or microphone.

11. <MIC IN> terminal

    Connects an external microphone (optional).

    - When using the phantom microphone, set to the [AUDIO] menu → [INPUT SETTINGS] → [FRONT MIC POWER] → [ON]. When it is set to [ON] and a microphone is not connected, low-frequency noise may occur. This is not a problem when a microphone is connected.

Top of the page