- Top
- Shooting
- Selecting audio input signal and adjusting recording level
- Selecting audio input signals

# Selecting audio input signals

Selects the audio signal to input to the audio channel 1 to 4 by <AUDIO IN CH1> to <AUDIO IN CH4> switch.

The audio input selection status can be checked on the AUDIO screen of the mode check display.

[AUDIO]

[MIC POWER(MENU)]

[ON]([FRONT]), [OFF]([REAR])

[VOL. SELECT]

[CH1/2]

[A.IN]

[LEVEL]

[F.VOL.]

[LIMITER]

[LOWCUT]

[CH1]

[FRONT]

[AUTO]

[OFF]

[OFF]

[CH2]

[FRONT]

[AUTO]

[OFF]

[OFF]

[CH3]

[REAR]

[AUTO]

[OFF]

[CH4]

[REAR]

[AUTO]

[OFF]

[CH1]

[CH2]

Top of the page