- Top
- Description of Parts
- Audio (output) function section

# Audio (output) function section

1. <MONITOR> dial

   Adjusts the volume of the monitor audio during playback, recording, and recording standby.

2. <ALARM> dial

   Adjusts the volume of the alarm from the built-in speaker and earphones.

   When set to the minimum position, the alarm cannot be heard.

3. Built-in speaker

   EE audio is output during recording, and playback audio is output during playback.

   An alarm sound is output in sync with flashing/lighting of the <WARNING> lamp or warning indicator.

   Audio from the built-in speaker is automatically muted when earphones are connected to the <PHONES> terminal.

4. <MONITOR SELECT> switch

   Selects audio output from the built-in speaker, earphones, and <AUDIO OUT> terminal interlocked with the audio channel selector switch.

   <CH1/3>: Outputs audio signal of the audio channel 1 or the audio channel 3.

   <ST>: Outputs the stereo audio signal of the audio channel 1 and the audio channel 2, or the audio channel 3 and the audio channel 4. Set to the MIX signal in the [AUDIO] menu → [OUTPUT SETTINGS] → [MONITOR SELECT] → [MIX].

   <CH2/4>: Outputs audio signal of the audio channel 2 or the audio channel 4.

   <MONITOR SELECT> switch | Audio channel selector switch
   --- | ---
   <CH1/2> | <CH3/4>
   <CH1/3> | Audio channel 1 | Audio channel 3
   <ST> | Stereo output from audio channels 1 and 2* | Stereo output from audio channels 3 and 4*
   <CH2/4> | Audio channel 2 | Audio channel 4

   Switches between [STEREO] and [MIX] in the [AUDIO] menu → [OUTPUT SETTINGS] → [MONITOR SELECT].

5. Audio channel selector switch

   Switches the audio channel output to the built-in speaker, earphones, and <AUDIO OUT> terminal.

   <CH1/2>: Outputs audio signal of the audio channel 1 and the audio channel 2.

   <CH3/4>: Outputs audio signal of the audio channel 3 and the audio channel 4.

6. <PHONES> terminal

   This is a stereo mini jack terminal for the audio monitor earphones.

   Same audio is output for both the front and the rear sides.

7. <AUDIO OUT> terminal

   Outputs the audio signal recorded in the audio channel 1 to audio channel 4.

   - The audio signal to be output is switched with the <MONITOR SELECT> switch.

Top of the page