- Top
- Shooting
- Convenient shooting functions
- Displaying zebra pattern

# Displaying zebra pattern

The camera can display two types of zebra patterns.

When the <ZEBRA> switch of the viewfinder is set to <ON>, the zebra pattern currently set in the menu is displayed on the viewfinder screen.

Zebra patterns can also be displayed in the video output from <SDI OUT1>/<SDI OUT2>/<HDMI> terminals according to settings.

The level for displaying zebra patterns can be set in the [VIDEO OUT/LCD/VF] menu → [EI ASSIST].

Item | Description of settings
--- | ---
[ZEBRA1 DETECT] | Sets the level of zebra pattern 1 tilting to the right. [0%]…[109%] (Factory setting: [80%])
[ZEBRA2 DETECT] | Sets the level of zebra pattern 2 tilting to the left. [0%]…[109%] (Factory setting: [100%])
[ZEBRA2] | Selects the type of [ZEBRA2]. [ON], [SPOT], [OFF] (Factory setting: [OFF])

[SPOT]: The image level from the setting value of [ZEBRA1 DETECT] to the setting value of [ZEBRA2 DETECT] is displayed in the zebra pattern.

[ZEBRA2]

Image level

[ON]

[OFF]

[SPOT]

[109%]

[ZEBRA2 DETECT]

[ZEBRA1 DETECT]

[0%]

When displaying the zebra pattern in the video output from <SDI OUT1> and <SDI OUT2> terminals, perform setting in the [VIDEO OUT/LCD/VF] menu → [SDI OUT1]/[SDI OUT2] → [SDI OUT ZEBRA].

Display of zebra pattern output to the <HDMI> terminal is based on the following setting.

- [VIDEO OUT/LCD/VF] menu → [HDMI OUT] → [SIGNAL SEL]

- [VIDEO OUT/LCD/VF] menu → [SDI OUT1]/[SDI OUT2] → [SDI OUT ZEBRA]

NOTE

- The zebra pattern is not displayed when the [SCENE FILE] menu → [GAMMA MODE SEL] → [HLG] is selected.

Top of the page