- Top
- Shooting
- Display of the viewfinder status
- Checking and displaying shooting status

# Checking and displaying shooting status

Setting and status of each function is always displayed in the camera image screen but they can be set to be displayed only when required.

Most of the set values and status will not be displayed when the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [INDICATOR SW] → [OFF] is selected.

When there is a need to confirm, push the <MARKER SEL>/<MODE CHECK> towards the <MCK> side while the camera image screen is displayed to display the STATUS screen of the mode check which show the shooting status.

For details about each item that can be displayed in the mode check, refer to “Mode check display”.

The following table indicates each item to display/hide in each screen.

- “✓” indicates displaying and “—” indicates hiding.

- You can select to display or hide each item in the [VIDEO OUT/LCD/VF] menu → [INDICATOR].

Confirm the display position during playback with the corresponding numbers in “Screen display during shooting”

No | Display item name | Menu item and selection of display/hide | Switching display/hide in the normal screen | Playback screen | STATUS
--- | --- | --- | --- | --- | ---
[INDICATOR SW]
[ON] | [OFF]
1 | Time code/User bits/Counter data | [TC] | ✓ | ✓ | — | ✓*1 | ✓
2 | Bonding Device Status | [BONDING DEVICE] | ✓ | ✓ | — | — | ✓
3 | Recording status | [REC STATUS] | ✓ | ✓ | ✓*2 | — | ✓
4 | Recording media | [REC MEDIA] | ✓ | ✓ | — | — | ✓
5 | Status of the card slot 1 or 2*3 | [SLOT STATUS] | ✓ | ✓ | —*4 | — | ✓
6 | Remaining capacity and status of the memory card in card slot 1 or 2*3 | [SLOT STATUS] | ✓ | ✓ | —*4 | — | ✓
7 | Message display area for wireless audio warning and cooling fan stop | [AUDIO] menu → [INPUT SETTINGS] → [WIRELESS WARN] | ✓ | ✓ | ✓ | — | ✓
|  | Fan stop message | — | ✓ | ✓ | ✓ | ✓
8 | SDI/HDMI remote control status | [REC REMOTE] | ✓ | ✓ | — | — | ✓
9 | Status of card slot 3 | [SLOT STATUS] | ✓ | ✓ | —*4 | — | ✓
10 | Remaining capacity and status of the memory card in card slot 3 | [SLOT STATUS] | ✓ | ✓ | —*4 | — | ✓
11 | Special recording function | [REC MODE] | ✓ | ✓ | — | — | ✓
12 | Two-slot function | [2 SLOTS FUNC.] | ✓ | ✓ | — | — | ✓
| [NDI|HX] | — | —
| Playback status | [PLAYBACK STATUS] | ✓ | — | — | ✓*1 | —
13 | Flash band compensation function | [FBC] | ✓ | ✓ | — | — | ✓
14 | Streaming status | [STREAMING] | ✓ | ✓ | — | — | ✓
15 | High dynamic range function/dynamic range stretcher function | [HDR/DRS] | ✓ | ✓ | — | — | ✓
16 | Connection status of the wireless LAN/wired LAN | [NETWORK] | ✓ | ✓ | — | — | ✓
17 | Remaining battery level | [BATTERY REMAIN] | ✓ | ✓ | —*4 | — | ✓
18 | Chromatic aberration compensation function | [CAC] | ✓ | ✓ | — | — | ✓
19 | Gamma mode | [GAMMA MODE] | ✓ | ✓ | — | — | ✓
20 | Scene file name | [SCENE FILE] | ✓ | ✓ | — | — | ✓
21 | Waveform monitor | Changing by USER switch | — | ✓ | ✓ | — | —
22 | Type of marker | — | — | — | — | — | ✓
23 | Digital zoom | [D.ZOOM] | ✓ | ✓ | — | — | ✓
24 | Focus | [ZOOM/FOCUS] | ✓ | ✓ | — | — | ✓
25 | Zoom | [ZOOM/FOCUS] | ✓ | ✓ | — | — | ✓
26 | Super black | [IRIS] | ✓ | ✓ | — | — | ✓
27 | Iris | [IRIS] | ✓ | ✓ | —*5 | — | ✓
28 | Super iris | [IRIS] | ✓ | ✓ | — | — | ✓
29 | High-sensitivity mode | [SHOOTING MODE] | ✓ | ✓ | — | — | ✓
30 | Iris override | [IRIS] | ✓ | ✓ | —*5 | — | ✓
31 | Luminance drop message display | — | — | ✓ | ✓ | — | ✓
32 | Luminance of Y GET | — | — | ✓ | ✓ | — | ✓
33 | Shutter speed | [SHUTTER] | ✓ | ✓ | — | — | ✓
34 | Date and time information | [DATE/TIME] | ✓ | ✓ | — | — | ✓
35 | Digital super gain | [GAIN] | ✓ | ✓ | — | — | ✓
36 | Gain | [GAIN] | ✓ | ✓ | — | — | ✓
37 | Auto knee | — | — | — | — | — | ✓
38 | Color temperature | [WHITE BALANCE] | ✓ | ✓ | —*6 | — | ✓
39 | Audio level meter | [AUDIO LEVEL METER] | ✓ | ✓ | — | — | ✓
40 | Filter position | [FILTER] | ✓ | ✓ | — | — | ✓
41 | Extender | [EXTENDER] | ✓ | ✓ | — | — | ✓
42 | Remote control status in an IP connection | — | — | — | — | — | ✓
43 | Error display of auto black balance | — | — | — | — | — | ✓
44 | Error display of auto white balance | — | — | — | — | — | ✓
45 | Message display area | — | — | ✓ | ✓ | ✓ | ✓
46 | Message for invalid filter position | — | — | ✓ | ✓ | — | ✓
47 | Clip name | [CLIP NAME] | ✓ | ✓ | — | ✓*1*7 | ✓
48 | Recording format | [REC FORMAT] | ✓ | ✓ | — | — | ✓
49 | System resolution/system frequency | [REC FORMAT] | ✓ | ✓ | — | — | ✓

Not displayed when the [VIDEO OUT/LCD/VF] menu → [INDICATOR] → [INDICATOR SW] → [OFF] is selected.

Only [REC] is displayed.

Status of the card slot 1 is displayed when the [RECORDING] menu → [REC MEDIA] is set to [expressP2], and the status of the card slot 2 is displayed when set to [microP2/SD].

Displayed when the remaining capacity of the memory card or remaining battery level gets low.

Displayed when the setting value of the iris override function is changed.

Displayed when the color temperature is changed with color temperature change function.

The display position differs in the playback screen. For details, refer to “Screen display during playback”.

Top of the page