- Top
- Shooting
- Setting the electronic shutter
- Shutter mode

# Shutter mode

The shutter modes available on the camera’s electronic shutter and shutter speeds that can be selected are as follows.

- Using a fixed shutter speed

  - When removing flicker caused by lighting

  - When shooting fast-moving subjects clearly

- Using the synchro scan mode

  - When shooting eliminating stripe patterns in the horizontal direction while shooting on the monitor screen

  - When shooting moving subjects with special effects

- Using the half shutter speed

  - When shooting with special effects such as films

[REC FORMAT]* | Shutter speed | Half shutter speed | Variable range of synchro scan mode
--- | --- | --- | ---
59.94p 59.94i | [1/100], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF] | 1/120 | 1/60.0 to 1/7200 | 3.0 deg to 360 deg (in 0.5 deg steps)
29.97p | 1/60 | 1/30.0 to 1/7200
23.98p | 1/48 | 1/24.0 to 1/7200
50.00p 50.00i | [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF] | 1/100 | 1/50.0 to 1/7200
25.00p | 1/50 | 1/25.0 to 1/7200

[REC FORMAT] indicates only frame rate. For example, [1080-59.94i/AVC-G50] is 59.94i, and [2160-29.97p/420LongGOP 100M] is 29.97p.

Top of the page