- Top
- Shooting
- Adjusting and setting the LCD monitor
- Using the LCD monitor

# Using the LCD monitor

Push the <OPEN> button towards the right to open the LCD monitor.

Set the LCD monitor screen to the easiest-to-view position.

Rotate up to 180° in the lens direction and 90° in the direction towards you.

Adjust the brightness of the LCD monitor/color density/contrast/brightness of the back light in the [VIDEO OUT/LCD/VF] menu → [LCD] → [BRIGHTNESS]/[COLOR LEVEL]/[CONTRAST]/[BACK LIGHT].

Brightness of the back light can be adjusted by pressing the USER button assigned with [LCD BACKLIGHT].

NOTE

- When closing the LCD monitor, be sure to close it firmly.

- Take care not to apply excessive force on the LCD monitor when it is opened. Doing so may result in a malfunction.

- Condensation sometimes forms on the LCD panel of the LCD monitor in locations subject to extreme temperature differences. If this happens, wipe with a soft, dry cloth.

- The LCD monitor will be slightly darker than normal immediately after the power is turned on when the camera is very cold. The brightness will return to normal when the internal temperature increases.

Top of the page