- Top
- Network Connection
- Using P2 Cast
- RTMP streaming from P2 Cast

# RTMP streaming from P2 Cast

- For detailed streaming procedure, refer to documents for P2 Cast.

- Remote control of the RTMP streaming is not possible when the menu or the thumbnail screen is displayed on the camera.

- Once the operation to start streaming from P2 Cast or setting of the destination URL is performed, the destination URL is recorded inside the camera. Streaming to the same destination can be performed with the operation from the camera after that. (Starting streaming with an operation on the camera)

- The recorded destination URL cannot be viewed on the camera.

- The recorded destination URL information is also cleared when the destination information is cleared.

  For details, refer to “Clearing the destination information”.

Top of the page