- Top
- Specification
- Specifications
- Audio input/output

# Audio input/output

<AUDIO IN CH1/3> terminal <AUDIO IN CH2/4> terminal | XLR×2, 3-pin <LINE>/<MIC>/<MIC+48V> (selected by switch) <LINE>: 4 dBu/0 dBu/−3 dBu (selected by menu) <MIC>: −40 dBu/−50 dBu/−60 dBu (selected by menu) <MIC+48V> + 48 V/OFF compatible
<MIC IN> terminal | XLR×1, 5-pin +48 V ON/OFF (selected by menu) −40 dBu/−50 dBu/−60 dBu (selected by menu)
Wireless slot | 25-pin, D-SUB, −40 dBu, 2ch supported
<AUDIO OUT> terminal | XLR×1, 5-pin 4 dBu/0 dBu/−3 dBu (selected by menu), equilibrium low impedance
<SDI OUT> terminal | LPCM 4ch
<HDMI> terminal | LPCM 2ch
<PHONES> terminal | 3.5 mm diameter stereo mini jack×2 (output impedance 100 Ω)
Built-in speaker | 20 mm diameter, round×1

Top of the page