- Top
- Specification
- Specifications
- Other input/output

# Other input/output

<GENLOCK IN> terminal | BNC×1, 1.0 V [p-p], 75 Ω
<TC IN/OUT> terminal | BNC×1 Used as input/output terminal (input/output switch by menu) Input: 0.5 V – 8.0 V [p-p], 10 kΩ Output: 2.0 V±0.5 V [p-p], low impedance
<DC IN> terminal | XLR×1, 4-pin, DC 12 V (DC 11.0 V – 17.0 V)
<DC OUT> terminal | 4-pin, DC 12 V (DC 11.0 V – 17.0 V), maximum output current 1.5 A
<LENS> terminal | 12-pin
<VF> terminal | 20-pin
<LAN> terminal | RJ-45 XLRnet connector: 1000BASE-T/100BASE-TX/10BASE-T
<USB2.0 HOST> terminal | Type A connector, 4-pin (5 V, 0.5 A), for attaching the wireless module (optional)
<USB DEVICE> terminal | USB 3.1 GEN1 type C connector, with USB mass storage function, without USB bus-powered function
<LIGHT> terminal | 2-pin, DC12 V (DC11.0 V – 17.0 V), maximum output current 4.5 A (up to 50 W equivalent)

Top of the page