- Top
- Description of Parts
- Warning and status display section

# Warning and status display section

1. <BRIGHT> button

   Controls the brightness of the display window.

   The brightness is switched in two levels every time the <BRIGHT> button is pressed.

   Regardless of the previous setting, it will display in dark setting when the power is turned on.

2. <WARNING> lamp

   Flashes or illuminates if something unusual occurs in the memory.

3. <STREAMING> lamp

   Illuminates in orange when the camera is streaming.

4. Back tally switch

   Controls the action of the back tally lamp and the rear tally lamp.

   <ON>: Enables the back tally lamp and the rear tally lamp.

   <OFF>: Disables the back tally lamp and the rear tally lamp.

5. Back tally lamp

   When the back tally switch is set to <ON>, the lamp acts in the same way as the front tally lamp at the viewfinder.

6. Rear tally lamp

   When the back tally switch is set to <ON>, the lamp acts in the same way as the back tally lamp.

Top of the page