- Top
- Specification
- Specifications
- Camera unit

# Camera unit

Pickup device | MOS×1
Number of pixels | 11.14 million pixels
Lens mount | 2/3-type bayonet
Optical filter | CC filter A: 3200 K, B: 4300 K, C: 5600 K, D: 6300 K ND filter 1: CLEAR, 2: 1/4ND, 3: 1/16ND, 4: 1/64ND
Gain setting | −6 dB to 30 dB: Can be set in 1 dB steps
Digital super gain (DS.GAIN) | Selectable from 6 dB, 10 dB, 12 dB, 15 dB, 20 dB, 24 dB, 28 dB, 34 dB
Super gain (S.GAIN) | Selectable from 30 dB, 36 dB, 42 dB
Shutter speed | When the [SYSTEM] menu → [FREQUENCY] → [59.94Hz] is set 1/100 sec., 1/120 sec., 1/250 sec., 1/500 sec., 1/1000 sec., 1/2000 sec., HALF When the [SYSTEM] menu → [FREQUENCY] → [50.00Hz] is set 1/60 sec., 1/120 sec., 1/250 sec., 1/500 sec., 1/1000 sec., 1/2000 sec., HALF
Synchro scan shutter | When the [SCENE FILE] menu → [SYNC SCAN TYPE] → [sec] is set When the [SYSTEM] menu → [FREQUENCY] → [59.94Hz] is set 59.94i/59.94p mode: 1/60.0 sec. to 1/7200 sec. 29.97p mode: 1/30.0 sec. to 1/7200 sec. 23.98p mode: 1/24.0 sec. to 1/7200 sec. When the [SYSTEM] menu → [FREQUENCY] → [50.00Hz] is set 50i/50p mode: 1/50.0 sec. to 1/7200 sec. 25p mode: 1/25.0 sec. to 1/7200 sec.
Shutter open angle | When the [SCENE FILE] menu → [SYNC SCAN TYPE] → [deg] is set 3.0 deg – 360.0 deg (can be set in 0.5 deg steps)
Sensitivity | When the [SYSTEM] menu → [SHOOTING MODE] → [NORMAL] is set F6 (2000 lx, 3200 K, 89.9% reflection, 59.94 Hz) F7 (2000 lx, 3200 K, 89.9% reflection, 50.00 Hz) When the [SYSTEM] menu → [SHOOTING MODE] → [HIGH SENS.] is set F10 (2000 lx, 3200 K, 89.9% reflection, 59.94 Hz) F11 (2000 lx, 3200 K, 89.9% reflection, 50.00 Hz)
Minimum subject illumination | Approx. 0.005 lx (F1.4, +42 dB (S.GAIN), +34 dB (DS.GAIN))
Image S/N | 62 dB (standard)
Horizontal resolution | UHD 2000 TV or higher (center) HD 1000 TV or higher (center)
Digital zoom | ×2, ×3, ×4

Top of the page