- Top
- Connecting to External Devices
- Connecting external devices and recording control function
- Confirming the control output status

# Confirming the control output status

The status of control is displayed in the viewfinder or the monitor screen when the control signal is output.

The displayed status is not the recording status of the connected external equipment, but the status of the control signal output from the camera.

Displays the control status of the recording start and recording stop on the external equipment connected to the <SDI OUT1>/<SDI OUT2>/<HDMI> terminals.

- [REC S/H]: Recording instruction is output to the output from the <SDI OUT1>/<SDI OUT2>/<HDMI> terminals.

- [S/H]: Pause instruction is output to the output from the <SDI OUT1>/<SDI OUT2>/<HDMI> terminals.

- [REC SDI]: Recording instruction is output to the output from the <SDI OUT1>/<SDI OUT2> terminals.

- [SDI]: Pause instruction is output to the output from the <SDI OUT1>/<SDI OUT2> terminals.

- [REC HDMI]: Recording instruction is output to the output from the <HDMI> terminal.

- [HDMI]: Pause instruction is output to the output from the <HDMI> terminal.

Top of the page