- Top
- Operation
- Menu settings
- [OTHERS] menu

# [OTHERS] menu

Configures the settings for writing/loading/initializing user files to the camera memory and other settings.

## [FILE]

Saves and loads the setting data.

For the saving and loading target, refer to “Target items for scene file/setup file/initialization”.

For details about saving and loading, refer to “Scene file”.

### [SCENE FILE(SD CARD)]

Loads or saves scene files on a memory card.

[LOAD] | Selects and loads the scene file saved on the memory card into the camera. Can select if all of the scene files ([F1:] to [F6:]) are loaded, or individually loaded.
[SAVE] | The setting values of the current scene file ([F1:] to [F6:]) are overwritten to the file selected from the list of scene files saved in the memory card.
[SAVE AS] | The setting values of the current scene file ([F1:] to [F6:]) is saved to the memory card as a new scene file by entering the file name.

### [SETUP FILE(SD CARD)]

Loads or saves setup files on a memory card.

[LOAD] | Selects the setup file saved on the memory card to load on the camera.
[SAVE] | Overwrites the file selected in the list of the setup files saved on the memory card with the current setting values of the camera.
[SAVE AS] | Enter a file name to save the current setting values in the camera as a new setup file in the memory card.

### [SETUP FILE(MEMORY)]

Loads or saves the setup files into the camera memory.

[LOAD] | Loads setup data saved on the memory.
[SAVE] | Saves the setup data to the memory.

### [CAC FILE(SD CARD)]

[LOAD] | Selects the chromatic aberration compensation data file saved in the memory card and loads it into the camera. Specifies the file number to save the chromatic aberration compensation data loaded from the memory card with [LOAD] into the camera.
[DELETE] | Selects and deletes the chromatic aberration compensation data file saved in the memory card.

### [LENS FILE(SD CARD)]

[LOAD] | Selects a lens file saved in the memory card, and loads it as one set of lens files (8-file set) into the camera memory.
[SAVE] | Overwrites a file selected from the list of lens files saved in the memory card with the one set of lens files (8-file set) in the camera memory.
[SAVE AS] | One set of lens files (8-file set) in the camera memory is saved in the memory card as a new lens file by entering a file name.

### [LENS FILE(MEMORY)]

[LOAD] | Selects the lens file saved in the camera memory, loads it, and uses it as current setting value for the operation.
[SAVE] | Current setting value is saved in the camera memory as a lens file by specifying the title and the file number.
[CLEAR ALL FILE] | Clears and initializes saved values for all the lens files.

### [SLOT FOR LOAD/SAVE]

Sets the card slot to load and save the scene file, setup file, CAC file, lens file, and streaming setting file.

The items that can be set are as follows.

- [SLOT2], [SLOT3]

(Factory setting: [SLOT2])

## [BATTERY]

### [DC IN SOURCE]

Sets the type of external power supply to input to the <DC IN> terminal.

The items that can be set are as follows.

[DC POWER SUPPLY] | Select when connecting the AC adaptor.
[BATTERY] | Select when connecting the battery. Voltage to display full/near end/end remaining capacity can be set in the [OTHERS] menu → [BATTERY] → [DC IN BATTERY].

(Factory setting: [DC POWER SUPPLY])

### [DC IN BATTERY]

[FULL VOLT] | Sets the voltage to display full remaining capacity when inputting an external battery from the <DC IN> terminal. The items that can be set are as follows. [13.0V] … [17.0V] (0.1 V steps) (Factory setting: [15.5V])
[NEAR END VOLT] | Sets the voltage to display near end remaining capacity when inputting an external battery from the <DC IN> terminal. The items that can be set are as follows. [11.1V] … [15.0V] (0.1 V steps) (Factory setting: [13.2V])
[END VOLT] | Sets the voltage to display end remaining capacity when inputting an external battery from the <DC IN> terminal. The items that can be set are as follows. [11.0V] … [14.9V] (0.1 V steps) (Factory setting: [12.5V])

### [ONBOARD BATTERY]

[BATTERY SEL] | Select according to the used battery. When set to [DIONIC], [HYTRON/TITON], [ENDURA], or [PAG], remaining capacity is detected and the warning is displayed according to the [NEAR END INFO] or the [END INFO] setting. The remaining capacity is detected by the voltage level when set to [other]. When there is no remaining capacity information, the remaining capacity is detected by the voltage level. The items that can be set are as follows. [DIONIC], [HYTRON/TITON], [ENDURA], [PAG], [other] (Factory setting: [DIONIC])
[FULL VOLT] | Sets the voltage to display full remaining capacity when the battery remaining capacity is detected by the voltage level. The items that can be set are as follows. [13.0V] … [17.0V] (0.1 V steps) (Factory setting: [15.5V])
[NEAR END VOLT] | Sets the voltage to display near end remaining capacity when the battery remaining capacity is detected by the voltage level. The items that can be set are as follows. [11.1V] … [15.0V] (0.1 V steps) (Factory setting: [13.2V])
[END VOLT] | Sets the voltage to display end remaining capacity when the battery remaining capacity is detected by the voltage level. The items that can be set are as follows. [11.0V] … [14.9V] (0.1 V steps) (Factory setting: [12.5V])
[NEAR END INFO] | Sets the percent value of the near end remaining capacity when the remaining capacity information is acquired from the battery. The items that can be set are as follows. [4%], [5%], [6%], [7%], [8%], [9%], [10%], [12%], [14%], [16%], [18%], [20%] (Factory setting: [5%])
[END INFO] | Sets the percent value of the end remaining capacity when the remaining capacity information is acquired from the battery. The items that can be set are as follows. [1%] … [10%] (1% steps) (Factory setting: [1%])

## [GENLOCK]

Switches the synchronization signal of the camera.

[INT] | Synchronizes to the internal standard signal regardless of the standard signal input to the <GENLOCK IN> terminal.
[GL IN] | Synchronizes to the standard signal input to the <GENLOCK IN> terminal.

(Factory setting: [INT])

### [H PHASE COARSE]

Performs coarse adjustment to match horizontal synchronization phase when building a system.

The items that can be set are as follows.

- [−100]…[100]

(Factory setting: [0])

### [H PHASE FINE]

Performs fine adjustment to match horizontal synchronization phase when building a system.

The items that can be set are as follows.

- [−100]…[100]

(Factory setting: [0])

## [COLOR BARS]

### [COLOR BARS TYPE]

Sets the color bar to be used.

[SMPTE] | Uses the color bars in SMPTE standard.
[FULL] | Uses the full color bars.

(Factory setting: [SMPTE])

NOTE

- A smear may occur depending on the output resolution.

### [TEST TONE]

Sets whether the audio test signal (tone signal with specification level 1 kHz) is output when the video is switched to the color bar.

The standard level varies depending on the setting of the [AUDIO] menu → [REC CH SETTINGS] → [HEAD ROOM].

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

## [LED]

### [REC TALLY]

Selects the method to display recording status at the camera.

[RED] | The red tally lamp illuminates.
[GREEN] | The green tally lamp illuminates. (Only in viewfinder)
[CHAR] | REC is displayed in characters in the viewfinder and the LCD monitor.

(Factory setting: [RED])

NOTE

- If set to [GREEN] or [CHAR], the front tally lamp, back tally lamp and rear tally lamp of the viewfinder do not illuminate while this camera is recording.

### [ACCESS LED]

Sets whether the card access lamp is to illuminate or not.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [LAN LED]

Sets whether to illuminate the LAN connector lamp.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [STREAMING LED]

Sets whether to illuminate the <STREAMING> lamp.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

## [CLOCK]

### [CLOCK SETTING]

Sets the calendar (date of the internal clock) and time.

Year | [2019]…[2037]
Month | [JAN]…[DEC] ([1]…[12])
Day | [1]…[31] ([28], [29], [30])
Hour | [0]…[23]
Minute | [0]…[59]

### [TIME ZONE]

Sets the time zone. It will switch to the time with the time difference added when the time zone setting is changed.

The items that can be set are as follows.

- [−12:00]…[+12:30] (30 minutes steps), [+12:45], [+13:00]

(Factory setting: [+0:00])

### [DATE FORMAT]

Sets the display order of the year, month, and date of the calendar (date of the internal clock). This is reflected to the date display of the clip information.

The items that can be set are as follows.

- [Y-M-D], [M-D-Y], [D-M-Y]

(Factory setting: [Y-M-D] (when [AREA SETTINGS] is set to [AREA 1]), [M-D-Y] (when [AREA SETTINGS] is set to [AREA 2]), [D-M-Y] (when [AREA SETTINGS] is set to [AREA 3] or [AREA 4]))

## [GPS]

Sets whether to enable the built-in GPS function.

Acquired position information is recorded in the shooting location of the metadata. The position information is not recorded in the metadata if the position information cannot be acquired.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

## [USB DEVICE]

### [CARD READER MODE]

Switches the camera to the card reader mode. A computer or other device can be connected via USB to use as a card reader of the memory card.

The LCD monitor turns off after approximately five to ten seconds when using the battery. Illuminates when the LCD monitor is touched.

It will return to the card reader mode screen when the cursor operation button is pressed or the jog dial button is turned.

Also, the card reader mode is ended and the camera image screen is displayed when the jog dial button or the <SET> button is pressed.

The items that can be selected are as follows.

- [YES], [NO]

### [SERVICE MODE]

Switches the camera to the service mode.

You can also check software information (licenses) on a computer and other equipment. Confirm “LICENSE.TXT” for the external drive recognized by a computer.

The LCD monitor turns off after approximately five to ten seconds when using the battery. Illuminates when the LCD monitor is touched.

It will return to the service mode screen when the cursor operation button is pressed or the jog dial button is turned.

Also, the service mode is ended and the camera image screen is displayed when the jog dial button or the <SET> button is pressed.

The items that can be selected are as follows.

- [YES], [NO]

## [INFORMATION]

### [VERSION]

Displays the information of the camera.

[MODEL] | Displays the product name of the camera.
[SERIAL NO.] | Displays the serial number of the camera.
[NETWORK ID(MAC ADDRESS)] | Displays the MAC address for the <LAN> terminal of the camera.
[VERSION] | Displays the firmware version of the camera.

### [OPERATION TIME]

[TOTAL OPERATION] | Displays the total operation time of the camera.

### [UPDATE]

Updates the firmware.

Insert the memory card where the update file is saved into card slot 2.

The items that can be selected are as follows.

- [YES], [NO]

## [LANGUAGE]

Sets the display language.

- When [AREA SETTINGS] is set to [AREA 1]

  [] | Japanese
  [English] | English

  (Factory setting: [English])

- When [AREA SETTINGS] is set to [AREA 2]

  [English] | English
  [Français] | French
  [Español] | Spanish

  (Factory setting: [English])

- When [AREA SETTINGS] is set to [AREA 3]

  [English] | English
  [Français] | French
  [Deutsch] | German
  [Español] | Spanish
  [Italiano] | Italian

  (Factory setting: [English])

- When [AREA SETTINGS] is set to [AREA 4]

  [English] | English
  [Français] | French
  [Español] | Spanish

  (Factory setting: [English])

## [MENU INITIALIZE]

Most of the setting values of the menu is returned to the factory setting status. The camera is restarted after executing.

Top of the page