- Top
- Preparation
- Mounting and adjusting the lens
- Adjusting lens flange back

# Adjusting lens flange back

If images are not clearly focused at both telephoto and wide-angle positions during zoom operations, adjust the flange back (distance from the lens mounting surface to the image formation surface).

Once adjusted, the flange back does not need to be readjusted until the lens is changed.

NOTE

- Refer to the lens operating instructions for guidance on adjustment methods and positions of lens parts.

Approximately 3 m

Mount the lens on the camera.

Make sure to connect the lens cable.

Set the lens iris to manual, and fully open the iris.

Place the flange back adjustment chart approximately 3 m from the lens and adjust the lighting on the chart to obtain an appropriate image output level.

If the image level is too high, use the filters or the shutter.

Loosen the F.f (Flange focus) ring clamping screw.

Set the zoom ring to the telephoto end position, either manually or by electric drive.

Aim the lens at the flange back adjustment chart and turn the distance ring to bring the chart into focus.

Set the zoom ring to the wide-angle end position and turn the F.f (Flange focus) ring to bring into focus.

At this time, do not move the distance ring.

Repeat steps 5 to 7 until the lens is in focus at both the telephoto and wide-angle positions.

Firmly tighten the F.f (Flange focus) ring clamping screw.

NOTE

- F.b (Lens flange back) ring may be indicated on some lenses as the F.f (Flange focus) ring.

Top of the page