- Top
- Network Connection
- Preparing for connection
- For the wireless module AJ-WM50

# For the wireless module AJ-WM50

Mount the wireless module AJ-WM50 (optional) to the camera.

<USB2.0 HOST> terminal

Open the <USB2.0 HOST> terminal cover.

Connect the wireless module to the <USB2.0 HOST> terminal.

Insert it all the way.

NOTE

- When removing the wireless module, pull it out straight.

## Cautions when using the wireless module AJ-WM50

Read the operating instruction of the wireless module thoroughly and understand it before using.

For the latest information, visit the following website:

https://pro-av.panasonic.net/

Top of the page