- Top
- Operation
- Menu settings
- [RECORDING] menu

# [RECORDING] menu

Sets the various items in the recording function.

## [FORMAT MEDIA]

Formats the memory card in the specified card slot. Data deleted as a result of formatting cannot be restored. Always confirm the data before formatting.

The items that can be selected are as follows.

- [SLOT1], [SLOT2], [SLOT3]

## [CLIP NAME]

### [CAM INDEX]

Sets the CAM INDEX used in the name for the MOV format file to be recorded. Set one upper case alphabetical character. This is used as a value to be stored in the volume label of the memory card.

The items that can be set are as follows.

- [A]…[Z]

(Factory setting: [A])

### [NEXT CARD COUNT]

Sets the CARD COUNT used in the name for the MOV format file to be recorded.

In the following cases, the setting value in [NEXT CARD COUNT] is stored in the volume label of the memory card together with the [CAM INDEX] setting value as CARD COUNT. Also, the setting value will increase one after storing. (It will return to [001] after [999])

- When formatted the memory card

- When recorded to the memory card where CARD COUNT is not stored in the volume label

The items that can be set are as follows.

- [001]…[999]

(Factory setting: [001])

## [REC MEDIA]

Selects the memory card to be recorded.

- Recording is not possible when a memory card with the format that is not selected is inserted.

[expressP2] | Use the expressP2 card in the card slot 1.
[microP2/SD] | Use the microP2 card or the SD card in the card slot 2 or the card slot 3.

(Factory setting: [microP2/SD])

## [FILE SPLIT]

Selects the split method of the file in P2 format to be recorded.

[ONE FILE] | Record as a single file on the expressP2 card or microP2 card with 32 GB or more. The recording format is AVC-Intra 422 or AVC-LongG.
[SPLIT] | The file is split in 4 GB units regardless of the recording format or the memory card.

(Factory setting: [SPLIT])

NOTE

- When using a microP2 card with 32 GB or less, it is split every 4 GB regardless of selected item.

- A clip of 4 GB or more recorded by selecting [ONE FILE] cannot be copied to a microP2 card with 32 GB or less.

## [2 SLOTS FUNC.]

Sets the recording function that uses card slots 2 and 3.

[OFF] | Does not set.
[RELAY REC] | Sets to the relay recording.
[SIMUL REC] | Sets to the simultaneous recording.

(Factory setting: [RELAY REC])

NOTE

- For the combinations and restrictions of the settings, refer to “Recording function that cannot be used simultaneously”.

## [PRE REC]

Sets whether to perform pre-recording.

The pre-recording time varies depending on the setting of the [SYSTEM] menu → [FILE FORMAT]/[REC FORMAT].

[ON] | Performs the pre-recording. The pre-recording time is as follows. When [FILE FORMAT] is set to [P2]: Approximately 3 seconds When [FILE FORMAT] is set to [MOV], and [REC FORMAT] is set to [2160-29.97p/422ALL-I 400M], [2160-25.00p/422ALL-I 400M], or [2160-23.98p/422ALL-I 400M]: Approximately 3 seconds When [FILE FORMAT] is set to [MOV], and [REC FORMAT] is set to [2160-59.94p/HEVC LongGOP 200M], [2160-59.94p/HEVC LongGOP 100M], [2160-59.94p/420LongGOP 150M], [2160-50.00p/HEVC LongGOP 200M], [2160-50.00p/HEVC LongGOP 100M], [2160-50.00p/420LongGOP 150M], [2160-29.97p/HEVC LongGOP 150M], [2160-29.97p/422LongGOP 150M], [2160-29.97p/420LongGOP 100M], [2160-25.00p/HEVC LongGOP 150M], [2160-25.00p/422LongGOP 150M], [2160-25.00p/420LongGOP 100M], [2160-23.98p/HEVC LongGOP 150M], [2160-23.98p/422LongGOP 150M], or [2160-23.98p/420LongGOP 100M]: Approximately 5 seconds When set to anything other than above: Approximately 10 seconds
[OFF] | Does not perform the pre-recording.

(Factory setting: [OFF])

NOTE

- For the combinations and restrictions of the settings, refer to “Recording function that cannot be used simultaneously”.

## [REC FUNCTION]

### [REC MODE]

Selects the recording mode.

[NORMAL] | Performs the standard recording.
[INTERVAL] | Performs the interval recording. (A function to repeatedly perform the operation of one frame recording in set interval.)

(Factory setting: [NORMAL])

NOTE

- For the combinations and restrictions of the settings, refer to “Recording function that cannot be used simultaneously”.

### [REC MODE HOLD]

Selects whether to hold [REC MODE] settings.

[ON] | Holds the settings.
[OFF] | Does not hold the settings. It will always be [NORMAL] the next time when the power is turned on.

(Factory setting: [OFF])

### [INTERVAL TIME]

Sets the interval duration for interval recording.

The items that can be set are as follows.

- [1s], [2s], [5s], [10s], [30s], [1min], [5min], [10min]

(Factory setting: [5min])

## [TC/UB]

### [DF/NDF]

Sets the count method for the time code generator.

Enabled only when the recording frame frequency of the [SYSTEM] menu → [REC FORMAT] is set to 59.94i/59.94p/29.97p.

[DF] | Uses the drop frame mode.
[NDF] | Uses the non-drop frame mode.

(Factory setting: [DF])

NOTE

- The setting is fixed to [NDF] when the [RECORDING] menu → [REC FUNCTION] → [REC MODE] → [INTERVAL] is set.

### [UB MODE]

Sets user bits. User bits are recorded in the clip. Also, it is output as LTC UB, VITC UB of the SDI signal.

[FRAME RATE] | Selects the image information (such as frame rate) of the camera.
[USER] | Selects the set user bits.
[TIME] | Selects the local time. (hh, mm, ss)
[DATE] | Selects the local date and time. (YY, MM, DD, hh)
[TC] | Records the time code value as user bits.
[CLIP NAME] | Records the value that CAM INDEX (one character) and CARD COUNT (three-digit number) are converted to ASCII character code. Only enabled when the [SYSTEM] menu → [FILE FORMAT] → [MOV] is set.

(Factory setting: [USER])

### [TC IN/OUT SEL]

Sets the input/output of the <TC IN/OUT> terminal.

[TC IN] | Sets to the time code input.
[TC OUT] | Sets to the time code output.

(Factory setting: [TC IN])

### [TC OUT REF]

Sets the output delay of the time code that is output from the <TC IN/OUT> terminal.

[RECORDING] | Outputs the recording time code without delay. This is used when performing simultaneous recording on two cameras with the time code of this camera as the master.
[SDI OUT1] | Matches to the output image from the <SDI OUT1> terminal. Outputs without delay when the image is not output from the <SDI OUT1> terminal.

(Factory setting: [RECORDING])

## [REC COUNTER]

Sets operation of the counter for recording.

[TOTAL] | Performs continuous counting until it is reset by pressing the <RESET> button.
[CLIP] | Clears the counter value at the start of recording and counts the time for each recording.

(Factory setting: [TOTAL])

Top of the page