- Top
- Connecting to External Devices
- Connecting external devices and recording control function
- Remote function

# Remote function

The signal to control the external equipment is superimposed in the output signal coupled with the operation of the <REC> button on the camera.

The control signals to start the recording and pause the recording are alternately output every time the <REC> button is pressed.

- Recording is performed on both the memory card and the external equipment by inserting a memory card into the camera and pressing the <REC> button.

- Recording is performed only in the external equipment when the <REC> button is pressed without inserting a memory card into the camera.

#### Outputting from the <SDI OUT1>/<SDI OUT2> terminal

This is enabled by the [VIDEO OUT/LCD/VF] menu → [SDI OUT1]/[SDI OUT2] → [SDI REC REMOTE] → [ON].

#### Outputting from the <HDMI OUT> terminal

This is enabled by the [VIDEO OUT/LCD/VF] menu → [HDMI OUT] → [HDMI REC REMOTE] → [ON].

NOTE

- The tally lamp is illuminated even when recording only on the external record.

- When the [OTHERS] menu → [LED] → [REC TALLY] → [GREEN]/[CHAR] is set, recording status of the camera is indicated with the green tally lamp on the viewfinder or with characters.

  With this setting, it can be distinguished from the control status of the external device indicated by the tally lamp.

- The SDI and HDMI remote functions are disabled for the interval recording.

Top of the page