- Top
- Description of Parts
- Power supply and accessory mounting section

# Power supply and accessory mounting section

1. Power switch

   Switches between power on/standby.

   To turn on, set the power switch to < > (ON). To set to standby, set the power switch to < > (standby).

   NOTE

   - Even when the power switch is set to the < > (standby) position, the camera is not shut off from the main power.

2. Viewfinder left/right positioning ring

   To adjust the left/right position of the viewfinder, loosen this ring, and slide the viewfinder to the left or right to adjust it to an easy-to-view position. After adjustment, turn in the <LOCK> direction and firmly clamp.

3. <VF> terminal

   Mount the viewfinder AG-CVF15G (optional), AJ-CVF50G (optional), etc.

4. Mount cap

   Raise the lens lever to remove the cap. Replace the cap when the lens is not mounted.

5. Cable holders

   Fix the cables for lens or microphone.

6. Lens mount

   Mounts the 2/3-inch bayonet lens.

7. Tripod mount

   Attaches the tripod adaptor SHAN-TM700 (optional). (bottom)

8. Lens lever

   After mounting the lens to the lens mount, tighten the lens lever to secure the lens.

9. <LIGHT> switch

   Select how to turn on/off the video light connected to the <LIGHT> terminal.

   <AUTO>: When the video light is left turned on, the light is illuminated at the same time that recording starts on the camera and goes out at the same time that recording stops.

   <MANUAL>: The light is illuminated according to whether the video light is turned on/off.

10. Viewfinder front/back positioning lever

    To adjust the front/back position of the viewfinder, loosen this lever, and slide the viewfinder to the front or back to adjust it to an easy-to-view position. After adjustment, turn in the <LOCK> direction and firmly clamp.

11. Shoulder strap mounting section

    Mounts the supplied shoulder strap. (Attaching the shoulder strap)

12. Battery release lever

    Used when removing the battery from the camera.

13. Battery holder

    Mounts the Anton/Bauer battery (optional).

14. <DC IN> terminal

    This is the input terminal for the external power supply. Connect to the external DC power supply.

15. <DC OUT> terminal

    This is the DC12 V power supply output terminal. It provides a maximum current of 1.5 A.

    NOTE

    - Make sure that polarity is correct before connecting an external device. Doing so may result in a malfunction.

16. Accessory mounting holes

    Attaches accessories.

    Do not attach anything other than an accessory.

    - Mounting hole size

      - 1/4-20 UNC (screw length 10 mm or shorter)

      - 3/8-16 UNC (screw length 10 mm or shorter)

17. Light shoe

    Attaches the video light, etc.

    - Mounting hole size

      1/4-20 UNC (screw length 6 mm or shorter)

18. <LIGHT> terminal

    Connect a video light 50 W or less.

    The remaining battery level drops sharply when the video light is illuminated. When using a video light, using a battery of 90 Wh or more is recommended.

19. Microphone holder mounting section

    Mounts the microphone holder AJ-MH800G (optional).

20. <LENS> terminal

    Connects the lens connection cable. For details of the lens used, refer to the Operating Instructions for the lens.

Top of the page