- Top
- Shooting
- Setting high dynamic range (HDR)
- Playing back the signal recorded in high dynamic range (HDR)

# Playing back the signal recorded in high dynamic range (HDR)

When set to the [SCENE FILE] menu → [GAMMA MODE SEL] → [HLG], detects the recorded information and sets as follows.

#### When recorded information is in high dynamic range

<SDI OUT1> terminal: Outputs in high dynamic range (HDR) or standard dynamic range (SDR) according to the setting of the [VIDEO OUT/LCD/VF] menu → [SDI OUT1] → [SDI OUT HDR].

<SDI OUT2> terminal: Outputs in high dynamic range (HDR) or standard dynamic range (SDR) according to the setting of the [VIDEO OUT/LCD/VF] menu → [SDI OUT2] → [SDI OUT HDR].

<HDMI> terminal: When set to the [VIDEO OUT/LCD/VF] menu → [HDMI OUT] → [SIGNAL SEL] → [SDI OUT1(2160p)], outputs according to the setting of the [VIDEO OUT/LCD/VF] menu → [SDI OUT1] → [SDI OUT HDR]. When set to [SDI OUT2], outputs according to the setting of the [VIDEO OUT/LCD/VF] menu → [SDI OUT2] → [SDI OUT HDR].

Viewfinder, LCD monitor: Outputs according to the setting of the [VIDEO OUT/LCD/VF] menu → [LCD/VF HDR]. HDR or SDR can be selected when recording in HDR.

#### When recorded information is not in high dynamic range or there is no recorded information

<SDI OUT1>/<SDI OUT2>/<HDMI> terminal, view finder, LCD monitor: Outputs the recorded video as is.

Following settings will be disabled: the [VIDEO OUT/LCD/VF] menu → [SDI OUT1]/[SDI OUT2] → [SDI OUT HDR], the [VIDEO OUT/LCD/VF] menu → [LCD/VF HDR].

NOTE

- For clips recorded with high dynamic range (hybrid log gamma), [HLG] is displayed for [GAMMA] item in detailed information about the clip displayed in the [THUMBNAIL] menu → [CLIP] → [INFORMATION].

- Recorded video will be output as is regardless of recorded information when anything other than the [SCENE FILE] menu → [GAMMA MODE SEL] → [HLG] is selected.

Top of the page