- Top
- Shooting
- Display of the viewfinder status
- Lamp display in the viewfinder

# Lamp display in the viewfinder

The example is for the AJ-CVF50G. (For information on the viewfinder, refer to the Operating Instructions for the optional viewfinder.)

1. Green tally lamp

   Lights up green if a green tally signal is received from the Camera Control Unit.

2. TALLY/REC (recording) lamp

   Illuminated in red during recording, and flashes if an abnormality occurs.

   For details, refer to “Warning system”.

3. [!] lamp

   [!] lamp of the viewfinder illuminates when the items set to [ON] in the [VIDEO OUT/LCD/VF] menu → [!LED] are enabled.

4. BATT (battery) lamp

   Starts flashing few minutes before the battery voltage drops and the battery charge runs out.

   It is illuminated after the battery is completely flat.

   To prevent operation from being interrupted, replace the battery before it is nearly flat.

   For details, refer to “Warning system”.

5. SAVE lamp

   The lamp is always out.

Top of the page