- Top
- Shooting
- Handling setting data
- Setting data file configuration

# Setting data file configuration

Scene files with [F1:] to [F6:] can be saved on the camera according to the settings in the main menu → [SCENE FILE].

Scene file data ([F1:] to [F6:]) can be saved as a file, and up to eight files can be saved on the SD memory card at a time, which can be loaded and used.

Setting menu values can be saved as one user file on the camera, and up to eight files can be saved on the SD memory card.

[USER MENU] settings registered with [USER MENU SEL] can also be saved on or loaded from the camera and the SD memory card at the same time as a user file.

Setting data file structure of the camera is as follows.

#### Scene file

The camera

SD memory card

(Factory settings)

[F1:]

[F2:]

[F3:]

[F4:]

[F5:]

[F6:]

Scene file 1

[F1:]

[F2:]

[F3:]

[F4:]

[F5:]

[F6:]

[F1:]

[F2:]

[F3:]

[F4:]

[F6:]

(Current value)

[F5:]

Scene file 8

[F1:]

[F2:]

[F3:]

[F4:]

[F5:]

[F6:]

[F3:]

[F5:]

[F6:]

[F4:]

[F1:]

[F2:]

(Value saved on the camera)

Select [INITIALIZE] in the main menu → [SCENE FILE] → [LOAD/SAVE/INITIALIZE].

By scene file unit as selected in the main menu → [SCENE FILE] → [FILE SELECT]

Select [LOAD] or [SAVE] in the main menu → [SCENE FILE] → [LOAD/SAVE/INITIALIZE].

By scene file unit as selected in the main menu → [SCENE FILE] → [FILE SELECT]

Select [LOAD] or [SAVE] in the main menu → [CARD FUNCTIONS] → [SCENE FILE].

[F1:] to [F6:] at once

#### User file

The camera

SD memory card

(Factory settings)

[USER FILE] (including [USER MENU])

User file 1

(Current value)

[USER FILE] (including [USER MENU])

User file 8

(Value saved on the camera)

[USER FILE] (including [USER MENU])

Select [INITIALIZE] in the main menu → [OTHER FUNCTIONS] → [USER FILE].

Select [LOAD] or [SAVE] in the main menu → [OTHER FUNCTIONS] → [USER FILE].

Select [LOAD] or [SAVE] in the main menu → [CARD FUNCTIONS] → [USER FILE].

Top of the page