- Top
- Shooting
- Adjustable settings when shooting
- Level gauge function

# Level gauge function

A level gauge that indicates the horizontal and vertical inclinations of the camera recorder can be displayed on the LCD monitor.

Horizontal direction

Example) When correcting the inclination towards the left

Vertical direction

Example) When correcting the downward inclination

Orange lines will be displayed when inclined. Orange lines will be changed to green lines when there is almost no inclination. Inclinations will be displayed up to approximately ±45° in the horizontal direction, and up to ±30° in the vertical direction.

Select [ON] in the main menu → [DISPLAY SETUP] → [LEVEL GAUGE].

NOTE

- The level gauge display is not recorded.

- The level gauge is not displayed in the viewfinder.

- The level gauge is not displayed when selecting [MIRROR] in the main menu → [DISPLAY SETUP] → [SELF SHOOT].

  The level gauge is not displayed when selecting [ON] in the main menu → [SYSTEM MODE] → [SCAN REVERSE].

- While moving the camera, the level gauge may not be displayed properly.

- When shooting while tilting the camera upward or downward greatly, the level gauge may not be displayed properly.

- When pressing the USER button where [LEVEL GAUGE] is assigned in the main menu → [USER SW], [ON] and [OFF] can be switched.

- When holding down the USER button where [LEVEL GAUGE RESET] is assigned in the main menu → [USER SW], the setting will be reset to the factory setting.

- When pressing the USER button where [LEVEL GAUGE RESET] is assigned in the main menu → [USER SW].

Top of the page