- Top
- Shooting
- Setting the time data
- Recording of time codes and user bits

# Recording of time codes and user bits

Recording of time codes

Setting | Recording TC
--- | ---
[LINE&FREQ] | [REC FORMAT] | [CAMERA MODE] | [FRAME RATE] | LTC | VITC
[1080-59.94P] | [AVC-I100/60P] [AVC-G25/60P] [AVC-G12/60P] | — | — | Recording run/free run* [DF]/[NDF] 30 frames | Same value as LTC
[AVC-I200/30PN] [AVC-G50/30PN] [AVC-G25/30PN] [AVC-G12/30PN] | — | Recording run/free run* [DF]/[NDF] 30 frames
[AVC-I100/30PN] | [30fps] | Recording run/free run* [DF]/[NDF] 30 valid frames
Other than [30fps] | Recording run [DF]/[NDF] 30 valid frames
[AVC-I200/24PN] [AVC-G50/24PN] [AVC-G25/24PN] [AVC-G12/24PN] | — | Recording run/free run* [NDF] 24 frames
[AVC-I100/24PN] | [24fps] | Recording run/free run* [NDF] 24 valid frames
Other than [24fps] | Recording run [NDF] 24 valid frames
[1080-59.94i] | [AVC-I200/60i] [AVC-I100/60i] [AVC-I50/60i] [AVC-G50/60i] [AVC-G25/60i] [AVC-G12/60i] | — | — | Recording run/free run* [DF]/[NDF] 30 frames | Same value as LTC
[DVCPRO HD/60i] | — | —
[1080-50P] | [AVC-I100/50P] [AVC-G25/50P] [AVC-G12/50P] | — | — | Recording run/free run* 25 frames | Same value as LTC
[AVC-I200/25PN] [AVC-G50/25PN] [AVC-G25/25PN] [AVC-G12/25PN] | — | Recording run/free run* 25 frames
[AVC-I100/25PN] | [25fps] | Recording run/free run* 25 frames
Other than [25fps] | Recording run 25 valid frames
[1080-50i] | [AVC-I200/50i] [AVC-I100/50i] [AVC-I50/50i] [AVC-G50/50i] [AVC-G25/50i] [AVC-G12/50i] | — | — | Recording run/free run* 25 frames | Same value as LTC
[DVCPRO HD/50i] | — | —
[1080-23.98PsF] | [AVC-I100/24PN] [AVC-G50/24PN] [AVC-G25/24PN] [AVC-G12/24PN] | — | — | Recording run/free run* [NDF] 24 frames | Same value as LTC
[720-59.94P] | [AVC-I200/60P] [AVC-I100/60P] [AVC-I100/30PN] [AVC-I50/60P] [AVC-G50/60P] [AVC-G25/60P] [AVC-G12/60P] | — | — | Recording run/free run* [DF]/[NDF] 30 frames | Same value as LTC
[DVCPRO HD/60P]
[AVC-I100/24PN] | — | — | Recording run/free run* 24 frames
[720-50P] | [AVC-I200/50P] [AVC-I100/50P] [AVC-I100/25PN] [AVC-I50/50P] [AVC-G50/50P] [AVC-G25/50P] [AVC-G12/50P] | — | — | Recording run/free run* 25 frames | Same value as LTC
[DVCPRO HD/50P]
[480-59.94i] | [DVCPRO50/60i] [DVCPRO/60i] [DV/60i] | [60i] | — | Recording run/free run* [DF]/[NDF] 30 frames | Same value as LTC (No recording in [DV/60i]/[DV/50i])
[30P] | —
[576-50i] | [DVCPRO50/50i] [DVCPRO/50i] [DV/50i] | [50i] | — | Recording run/free run* 25 frames | Same value as LTC (No recording in [DV/60i]/[DV/50i])
[25P] | —

For free run, the time code is slaved to the input TC of the <TC IN/OUT> terminal.

Output of time codes

Setting | Output TC
--- | ---
[LINE&FREQ] | [REC FORMAT] | [CAMERA MODE] | [FRAME RATE] | TC OUT | LTC, VITC of HD SDI
[1080-59.94P] | [AVC-I100/60P] [AVC-G25/60P] [AVC-G12/60P] | — | — | LTC is output. | LTC is output.
[AVC-I200/30PN] [AVC-G50/30PN] [AVC-G25/30PN] [AVC-G12/30PN] | — | LTC is output. | LTC is output.
[AVC-I100/30PN] | [30fps] | LTC is output. | LTC is output.
Other than [30fps] | Matches to the recording TC at the top of recording. 30 frames/second | Matches to the recording TC at the top of recording. 30 frames/second
[AVC-I200/24PN] [AVC-G50/24PN] [AVC-G25/24PN] [AVC-G12/24PN] | — | LTC is converted to 30 frames and output. | LTC is output.
[AVC-I100/24PN] | [24fps] | LTC is converted to 30 frames and output. | LTC is output.
Other than [24fps] | Matches to the recording TC at the top of recording. 30 frames/second | Matches to the recording TC at the top of recording. 30 frames/second
[1080-59.94i] | [AVC-I200/60i] [AVC-I100/60i] [AVC-I50/60i] [AVC-G50/60i] [AVC-G25/60i] [AVC-G12/60i] | — | — | LTC is output. | LTC is output.
[DVCPRO HD/60i] | — | —
[1080-50P] | [AVC-I100/50P] [AVC-G25/50P] [AVC-G12/50P] | — | — | LTC is output. | LTC is output.
[AVC-I200/25PN] [AVC-G50/25PN] [AVC-G25/25PN] [AVC-G12/25PN] | — | LTC is output. | LTC is output.
[AVC-I100/25PN] | [25fps] | LTC is output. | LTC is output.
Other than [25fps] | Matches to the recording TC at the top of recording. 25 frames/second | Matches to the recording TC at the top of recording. 25 frames/second
[1080-50i] | [AVC-I200/50i] [AVC-I100/50i] [AVC-I50/50i] [AVC-G50/50i] [AVC-G25/50i] [AVC-G12/50i] | — | — | LTC is output. | LTC is output.
[DVCPRO HD/50i] | — | —
[1080-23.98PsF] | [AVC-I200/24PN] [AVC-I100/24PN] [AVC-G50/24PN] [AVC-G25/24PN] [AVC-G12/24PN] | — | — | LTC is output. | LTC is output.
[720-59.94P] | [AVC-I200/60P] [AVC-I100/60P] [AVC-I100/30PN] [AVC-I50/60P] [AVC-G50/60P] [AVC-G25/60P] [AVC-G12/60P] | — | — | LTC is output. | LTC is output.
[DVCPRO HD/60P]
[AVC-I100/24PN] | — | — | LTC is converted to 30 frames and output. | LTC is converted to 30 frames and output.
[720-50P] | [AVC-I200/50P] [AVC-I100/50P] [AVC-I100/25PN] [AVC-I50/50P] [AVC-G50/50P] [AVC-G25/50P] [AVC-G12/50P] | — | — | LTC is output. | LTC is output.
[DVCPRO HD/50P]
[480-59.94i] | [DVCPRO50/60i] [DVCPRO/60i] [DV/60i] | [60i] | — | LTC is output. | None
[30P] | —
[576-50i] | [DVCPRO50/50i] [DVCPRO/50i] [DV/50i] | [50i] | — | LTC is output. | None
[25P] | —

Recording of user bits

Setting | Recording UB
--- | ---
[LINE&FREQ] | [REC FORMAT] | [CAMERA MODE] | [FRAME RATE] | LTC UB | VITC UB
[1080-59.94P] | [AVC-I100/60P] [AVC-G25/60P] [AVC-G12/60P] | — | — | Follows [UBG MODE].*1 | Follows [VITC UBG MODE].*2
[AVC-I200/30PN] [AVC-G50/30PN] [AVC-G25/30PN] [AVC-G12/30PN] | — | Frame information lock
[AVC-I100/30PN] | [30fps]
Other than [30fps]
[AVC-I200/24PN] [AVC-G50/24PN] [AVC-G25/24PN] [AVC-G12/24PN] | —
[AVC-I100/24PN] | [24fps]
Other than [24fps]
[1080-59.94i] | [AVC-I200/60i] [AVC-I100/60i] [AVC-I50/60i] [AVC-G50/60i] [AVC-G25/60i] [AVC-G12/60i] | — | — | Follows [UBG MODE].*1 | Follows [VITC UBG MODE].
[DVCPRO HD/60i] | — | —
[1080-50P] | [AVC-I100/50P] [AVC-G25/50P] [AVC-G12/50P] | — | — | Follows [UBG MODE].*1 | Follows [VITC UBG MODE].*2
[AVC-I200/25PN] [AVC-G50/25PN] [AVC-G25/25PN] [AVC-G12/25PN] | — | Frame information lock
[AVC-I100/25PN] | [25fps] | Frame information lock
Other than [25fps]
[1080-50i] | [AVC-I200/50i] [AVC-I100/50i] [AVC-I50/50i] [AVC-G50/50i] [AVC-G25/50i] [AVC-G12/50i] | — | — | Follows [UBG MODE].*1 | Follows [VITC UBG MODE].
[DVCPRO HD/50i] | — | —
[1080-23.98PsF] | [AVC-I200/24PN] [AVC-I100/24PN] [AVC-G50/24PN] [AVC-G25/24PN] [AVC-G12/24PN] | — | — | Follows [UBG MODE].*1 | Frame information lock
[720-59.94P] | [AVC-I200/60P] [AVC-I100/60P] [AVC-I100/30PN] [AVC-I100/24PN] [AVC-I50/60P] [AVC-G50/60P] [AVC-G25/60P] [AVC-G12/60P] | — | — | Follows [UBG MODE].*1 | Frame information lock
[DVCPRO HD/60P]
[720-50P] | [AVC-I200/50P] [AVC-I100/50P] [AVC-I100/25PN] [AVC-I50/50P] [AVC-G50/50P] [AVC-G25/50P] [AVC-G12/50P] | — | — | Follows [UBG MODE].*1 | Frame information lock
[DVCPRO HD/50P]
[480-59.94i] | [DVCPRO50/60i] [DVCPRO/60i] [DV/60i] | [60i] | — | Follows [UBG MODE].*1 | Follows [VITC UBG MODE].*3
[30P] | —
[576-50i] | [DVCPRO50/50i] [DVCPRO/50i] [DV/50i] | [50i] | — | Follows [UBG MODE].*1 | Follows [VITC UBG MODE].*3
[25P] | —

With [EXT], UB of the <TC IN/OUT> terminal is slaved.

During standard variable frame rate recording, frame rate information will be fixed.

When [CAMERA MODE] is set to [30P] and [25P], frame rate information will be fixed.

Output of user bits

Setting | Output UB
--- | ---
[LINE&FREQ] | [REC FORMAT] | [CAMERA MODE] | [FRAME RATE] | UB for TC OUT | LTC UB for HD SDI | VITC UB for HD SDI
[1080-59.94P] | [AVC-I100/60P] [AVC-G25/60P] [AVC-G12/60P] | — | — | LTC UB is output. | LTC UB is output. | VITC UB is output.
[AVC-I200/30PN] [AVC-G50/30PN] [AVC-G25/30PN] [AVC-G12/30PN] | —
[AVC-I100/30PN] | [30fps]
Other than [30fps]
[AVC-I200/24PN] [AVC-G50/24PN] [AVC-G25/24PN] [AVC-G12/24PN] | — | Outputs along to over 60P, based on LTC UB. | Outputs along to over 60P, based on LTC UB.
[AVC-I100/24PN] | [24fps]
Other than [24fps]
[1080-59.94i] | [AVC-I200/60i] [AVC-I100/60i] [AVC-I50/60i] [AVC-G50/60i] [AVC-G25/60i] [AVC-G12/60i] | — | — | LTC UB is output. | LTC UB is output. | VITC UB is output.
[DVCPRO HD/60i] | — | —
[1080-50P] | [AVC-I100/50P] [AVC-G25/50P] [AVC-G12/50P] | — | — | LTC UB is output. | LTC UB is output. | VITC UB is output.
[AVC-I200/25PN] [AVC-G50/25PN] [AVC-G25/25PN] [AVC-G12/25PN] | —
[AVC-I100/25PN] | [25fps]
Other than [25fps]
[1080-50i] | [AVC-I200/50i] [AVC-I100/50i] [AVC-I50/50i] [AVC-G50/50i] [AVC-G25/50i] [AVC-G12/50i] | — | — | LTC UB is output. | LTC UB is output. | VITC UB is output.
[DVCPRO HD/50i] | — | —
[1080-23.98PsF] | [AVC-I200/24PN] [AVC-I100/24PN] [AVC-G50/24PN] [AVC-G25/24PN] [AVC-G12/24PN] | — | — | LTC UB is output. | LTC UB is output. | VITC UB is output.
[720-59.94P] | [AVC-I200/60P] [AVC-I100/60P] [AVC-I100/30PN] [AVC-I50/60P] [AVC-G50/60P] [AVC-G25/60P] [AVC-G12/60P] | — | — | LTC UB is output. | LTC UB is output. | VITC UB is output.
[DVCPRO HD/60P]
[AVC-I100/24PN] | — | — | Outputs along to over 60P, based on LTC UB. | Outputs along to over 60P, based on LTC UB. | VITC UB is output.
[720-50P] | [AVC-I200/50P] [AVC-I100/50P] [AVC-I100/25PN] [AVC-I50/50P] [AVC-G50/50P] [AVC-G25/50P] [AVC-G12/50P] | — | — | LTC UB is output. | LTC UB is output. | VITC UB is output.
[DVCPRO HD/50P]
[480-59.94i] | [DVCPRO50/60i] [DVCPRO/60i] [DV/60i] | [60i] | — | LTC UB is output. | None | None
[30P] | —
[576-50i] | [DVCPRO50/50i] [DVCPRO/50i] [DV/50i] | [50i] | — | LTC UB is output. | None | None
[25P] | —

Top of the page