- Top
- Shooting
- Special recording functions
- Shot mark recording function

# Shot mark recording function

Shot mark is the mark added to the thumbnail of each clip to distinguish that clip from others.

Only clips with shot marks attached can be displayed or played back.

## Adding shot marks

Assign [SHOT MARK] to one of [USER1] to [USER8] in the main menu → [USER SW].

During recording or a pause after recording, press the button to which the shot mark is assigned.

- [MARK ON] is displayed, and the shot mark is added to the most recently recorded clip.

- Another press of the button displays [MARK OFF] and the shot mark disappears.

NOTE

- When the shot mark is added during a recording pause, it is added to the clip recorded immediately before.

- Shot marks can also be added while the thumbnail is being displayed. (Shot mark)

- Shot marks cannot be added during loop recording, interval recording, or one-shot recording. If an operation is invalid, [SHOT MARK INVALID] is displayed when the button is pressed.

- During playback, setting or canceling the shot mark is not available. While pausing the playback, setting or canceling the shot mark is available.

- The following restrictions apply when adding shot marks to combined clips, such as those recorded over multiple microP2 memory cards, or when deleting them.

  - All microP2 memory cards composed of clips must be inserted into the slots.

  - A shot mark is added only to the top clip among combined clips.

Top of the page