- Top
- Shooting
- Adjustable settings when shooting
- Macro

# Macro

Macro function can be switched [ON]/[OFF].

Press the USER button to which [FOCUS MACRO] has been assigned.

- When [ON] is set, is displayed at the top of the focus display on the viewfinder or LCD monitor.

- The operation mode when [ON] is set can be made in the main menu → [SW MODE] → [MACRO MODE].

- Only the wide macro area is enabled when [MACRO MODE] is set to [WIDE]. The minimum object distance (M.O.D) is maintained to be 1.1 m when the zoom position is within the tele macro area.

- Tele macro area and wide macro area are enabled when [MACRO MODE] is set to [ALL].

Top of the page