- Top
- Menu Operations
- Menu list
- [OTHER FUNCTIONS]

# [OTHER FUNCTIONS]

Configure these items to make settings for reading/writing, initialization of user file data on the internal memory, and the camera settings.

Item | Description of settings
--- | ---
[USER FILE] | Loads/saves/initializes user files on the camera memory. [LOAD]: Loads user files. [SAVE]: Saves user files. [INITIALIZE]: Restores user files to the factory settings.
[ACCESS LED] | Selects whether to light the access LED of the P2 card. [ON], [OFF] Factory setting: [ON]
[TALLY LAMP] | Sets up the tally lamp lighting conditions. [FRONT]: The front tally lamp lights up. [REAR]: The rear tally lamp lights up. [BOTH]: Both the front and rear tally lamps light up. [OFF]: The tally lamp does not light up. Factory setting: [OFF]
[CLOCK SETTING] | Sets the built-in calendar (date and time) and time zone.
[TIME ZONE] | For GMT, set using 30 minute intervals from −12:00 to +13:00 (however, +12:45 is possible). After setting the time, when changing the setting value for [TIME ZONE], the displayed and registered times switch to the time with the time difference.
[GL PHASE] | When in HD (1080i, 720P) mode, selects the output signal of phase to be locked to the signal input to the <GENLOCK IN/VIDEO OUT> terminal. [HD SDI]: Locks the HD SDI output signal to genlock input. [COMPOSITE]: Locks the down-converted composite output signals (signal from the <GENLOCK IN/VIDEO OUT> terminal and 480i, 576i signals from the <SDI OUT> terminal) to genlock input. Factory setting: [HD SDI]
[H PHASE] | Adjusts the horizontal phase when the phase is to be locked to the signal input to the <GENLOCK IN/VIDEO OUT> terminal. [−512]…[512] Factory setting: [0]
[SEEK POS SEL] | Selects the position to move when the <>/<> button is pressed while playback is paused. [CLIP]: Top of the clip [CLIP&TEXT MEMO]: Top of the clip and text memo location Factory setting: [CLIP]
[GPS] | Sets the GPS. Acquired position information is recorded in the shooting location of the metadata. [INTERNAL]: Activates the built-in GPS operation. The position information is output to the signal from the <SDI OUT> terminal. [EXTERNAL]: Acquires the position information from the external device connected to the camera via network. [OFF]: Does not activate the GPS operation. Does not output and record the location information. Factory setting: [OFF]
[P.OFF GPS DATA] | Retains the GPS location information when the camera is turned off. Sets whether to record the retained data at the next turning on until a positioning is performed. [HOLD]: Retains and records data. [CLEAR]: Clears the data at the time when the camera is turned off. Records 0 (No-Info) at the next turning on until a positioning is performed. Factory setting: [CLEAR]
[MENU INITIALIZE] | Restores the whole setting menu including all scene files (1 to 6) and user files to the factory settings.

Top of the page