- Top
- Shooting
- Adjusting image quality
- Color correction function

# Color correction function

This function sets color saturation and phase. It applies individual effect on 15 phases in a image. It can be set to individual color hue.

[(PHASE)]

[(SAT)]

#### General settings

Use the camera with the factory settings.

#### Advanced settings

[R (PHASE)]/[R-R-Mg (PHASE)]/[R-Mg (PHASE)]/[Mg (PHASE)]/[Mg-B (PHASE)]/[B (PHASE)]/[B-Cy (PHASE)]/[Cy (PHASE)]/[Cy-G (PHASE)]/[G (PHASE)]/[G-Yl (PHASE)]/[Yl (PHASE)]/[Yl-Yl-R (PHASE)]/[Yl-R (PHASE)]/[Yl-R-R (PHASE)]: Changes the phases. + makes it rotate clockwise, and − makes it rotate counter-clockwise.

[R (SAT)]/[R-R-Mg (SAT)]/[R-Mg (SAT)]/[Mg (SAT)]/[Mg-B (SAT)]/[B (SAT)]/[B-Cy (SAT)]/[Cy (SAT)]/[Cy-G (SAT)]/[G (SAT)]/[G-Yl (SAT)]/[Yl (SAT)]/[Yl-Yl-R (SAT)]/[Yl-R (SAT)]/[Yl-R-R (SAT)]: Changes the saturation.

Top of the page