- Top
- Connecting to External Devices
- Connecting to the remote operation panel (AK-HRP200G)
- Remote control unit connected to the camera

# Remote control unit connected to the camera

When AK-HRP200G is connected to the camera, the AK-HRP200G button’s operations are as follows:

#### Skin tone detail button (<SKINDTL>)

Operation varies depending on the lighting status of the button.

- When the button lights up, the operation follows the menu setting value of the camera (setting for skin tone detail).

- When the button lights off, the skin tone detail function is set to [OFF], regardless of the menu setting value of the camera.

After restarting the camera, the menu setting value is reflected in AK-HRP200G.

However, this function does not operate when the camera and AK-HRP200G have a serial connection.

#### Knee OFF button (<KNEE OFF>)

Operation varies depending on the lighting status of the button.

- When the button lights up, the knee function is set to [OFF], regardless of the menu setting value of the camera.

- When the button lights off, the operation follows the menu setting value of the camera (setting for the knee function).

After restarting the camera, the menu setting value is reflected in AK-HRP200G.

#### Matrix button (<MATRIX>)

When the button lights up, the menu setting value of the camera is always applied (setting for matrix). The function cannot be turned [OFF] even if the button is pressed.

After restarting the camera, the menu setting value is reflected in AK-HRP200G.

#### Scene file selection buttons (<SCENE1> - <SCENE4>)

Not supported.

#### User file selection buttons (<USER1> - <USER3>)

You can select the camera’s scene file F1 to F3. F4 to F6 cannot be selected.

However, this function does not operate when the camera and AK-HRP200G have a serial connection.

#### R flare/pedestal volume (<FLARE/PED R>), B flare/pedestal volume (<FLARE/PED B>)

Flare adjustment is not supported. Works only with the pedestal.

#### Adjusted value display area (4 digits)

Display of CC filter, zoom, and focus values are not supported.

#### Character/menu button (<CHARA/MENU>)

The status and menu are displayed in the output image from the <SDI OUT>, <HDMI OUT>, and <GENLOCK IN/VIDEO OUT> terminals regardless of camera’s menu setting value.

#### Sense volume (<SENSE>)

Zoom/focus speed can be adjusted.

- Turning it to the right accelerates the zoom/focus speed.

- Turning it to the left decelerates the zoom/focus speed.

#### ND filter/CC filter display selection button <ND/CC>

- Zoom mode and focus mode can be switched.

  Press the display selection button, and select either zoom mode or focus mode.

  - During zoom mode, the adjusted value display area (4 digits) shows [Zo].

  - During focus mode, the adjusted value display area (4 digits) shows [Fo].

    While the selection is displayed, you can change the adjusted value using the data set button (up) <UP>/data set button (down) <DOWN>.

- Auto focus and manual focus can be switched.

  Press the display selection button, and select the adjusted value display area (4 digits) [AF.]. While the selection is displayed, select auto focus or manual focus by pressing the data set button (up) <UP> or data set button (down) <DOWN>.

  - During manual focus, [AF.of] is displayed.

  - During auto focus, [AF.on] is displayed.

- During frame rate mode, the adjusted value display area (4 digits) shows [Frof], but it does not operate on the camera.

#### Data set button (up) <UP>

Zooms in during zoom mode.

You can adjust focus (on the back) during focus mode.

#### Data set button (down) <DOWN>

Zooms out during zoom mode.

You can adjust focus (on the front) during focus mode.

#### Selection dial <SELECT>

You can adjust focus during zoom mode. Turning the dial to the right focuses on the back. Turning the dial to the left focuses on the front.

You can adjust zoom during focus mode. Turning the dial to the right performs zoom in, and turning the dial to the left performs zoom out.

Top of the page