- Top
- Network Connection
- Preparing for connection
- For the wireless module AJ-WM30/AJ-WM50

# For the wireless module AJ-WM30/AJ-WM50

Connect the wireless module AJ-WM30/AJ-WM50 (optional) to the camera. The grip belt can be removed.

<OPEN> button

<USB2.0 HOST> terminal

Fig. 1

Fig. 2

Fig. 3

Press the <OPEN> button and remove the cover by sliding it in the direction of the arrow. (Fig. 1)

Connect the wireless module to the <USB2.0 HOST> terminal. (Fig. 2)

Insert it all the way.

Place the (AJ-WM50 only) module holder under the wireless module. (Fig. 3)

- Mount the cap of the wireless module to the hole of the module holder.

Slide the removed cover to close it.

NOTE

- When removing the wireless module, pull it down straight.

- When using a wireless module other than AJ-WM30/AJ-WM50, refer to “For wireless module other than AJ-WM30/AJ-WM50”.

## Storing the wireless module AJ-WM30

The removed wireless module AJ-WM30 can be stored in the grip belt.

## Cautions when using wireless module AJ-WM30/AJ-WM50

Read the operating manual of the wireless module thoroughly and understand it before using.

For the latest information, visit the following website:

https://pro-av.panasonic.net/

Top of the page