- Top
- Menu Operations
- Menu list
- [AUDIO SETUP]

# [AUDIO SETUP]

Configure the settings regarding audio input/output.

Item | Description of settings
--- | ---
[INPUT SETTING] | [INT MIC] | Sets built-in microphone on/off and selects the directionality. [STEREO]: Records audio from two directions in the front with the stereo microphone. [MONO]: This mode records clearer audio from the front by enhancing the directionality forward like a shotgun microphone. Audio recorded on the left and right are the same. [OFF]: Disables audio of the built-in stereo microphone. Factory setting: [STEREO]
| [INPUT1 MIC LEVEL] | Sets the level of an external microphone connected to the <AUDIO INPUT 1> terminal. Enabled only when a microphone is connected. [−40dB], [−50dB], [−60dB] Factory setting: [−50dB]
| [INPUT2 MIC LEVEL] | Sets the level of an external microphone connected to the <AUDIO INPUT 2> terminal. Enabled only when a microphone is connected. [−40dB], [−50dB], [−60dB] Factory setting: [−50dB]
| [INPUT1 LINE LEVEL] | Sets the level of an external line input to be connected to the <AUDIO INPUT 1> terminal. Enabled only for externally connected devices. [4dB], [0dB] Factory setting: [0dB]
| [INPUT2 LINE LEVEL] | Sets the level of an external line input to be connected to the <AUDIO INPUT 2> terminal. Enabled only for externally connected devices. [4dB], [0dB] Factory setting: [0dB]
[RECORDING CH SETTING] | [FRONT VR SELECT] | Sets the allocation to the <F.AUDIO LEVEL> dial. Enabled when the setting is other than <AUTO>. [0dB] to [−] can be adjusted. [CH1], [CH2], [CH3], [CH4], [CH1/CH2], [CH3/CH4], [ALL], [OFF] Factory setting: [OFF]
| [AUTO LEVEL CH3] | Selects the level setting method for audio channel 3. [ON]: Sets the mode to adjust automatically. The limiter does not work. [OFF]: The audio level follows the value for [LEVEL CONTROL CH3]. Factory setting: [ON]
| [AUTO LEVEL CH4] | Selects the level setting method for audio channel 4. [ON]: Sets the mode to adjust automatically. The limiter does not work. [OFF]: The audio level follows the value for [LEVEL CONTROL CH4]. Factory setting: [ON]
| [LEVEL CONTROL CH3] | Can be manually adjusted with this item when automatic level adjustment of audio channel 3 is [OFF]. [0]…[100] Factory setting: [70]
| [LEVEL CONTROL CH4] | Can be manually adjusted with this item when automatic level adjustment of audio channel 4 is [OFF]. [0]…[100] Factory setting: [70]
| [MIC LOWCUT CH1] | Enables/disables the lowcut filter for audio channel 1. [ON], [OFF] Factory setting: [OFF]
| [MIC LOWCUT CH2] | Enables/disables the lowcut filter for audio channel 2. [ON], [OFF] Factory setting: [OFF]
| [MIC LOWCUT CH3] | Enables/disables the lowcut filter for audio channel 3. [ON], [OFF] Factory setting: [OFF]
| [MIC LOWCUT CH4] | Enables/disables the lowcut filter for audio channel 4. [ON], [OFF] Factory setting: [OFF]
| [LIMITER CH1] | Enables/disables the limiter for audio channel 1. [ON], [OFF] Factory setting: [OFF]
| [LIMITER CH2] | Enables/disables the limiter for audio channel 2. [ON], [OFF] Factory setting: [OFF]
| [LIMITER CH3] | Enables/disables the limiter for audio channel 3. [ON], [OFF] Factory setting: [OFF]
| [LIMITER CH4] | Enables/disables the limiter for audio channel 4. [ON], [OFF] Factory setting: [OFF]
| [HEADROOM] | Sets the headroom (standard level). [12dB], [18dB], [20dB]
[OUTPUT SETTING] | [AUDIO OUT] | Sets the audio signal output from the <AUDIO OUT> terminal, headphone terminal, <HDMI OUT>terminal, and built-in speaker. [CH1/2], [CH1], [CH2], [CH3/4], [CH3], [CH4] Factory setting: [CH1/2]
| [TEST TONE] | Outputs rated level 1 kHz tone signal according to the reference level. The standard level varies depending on the setting of [HEADROOM]. [ON], [OFF] Factory setting: [ON]

Top of the page