- Top
- Menu Operations
- Menu list
- [AUTO SW]

# [AUTO SW]

Configure the settings regarding the auto mode.

Auto iris, auto gain control, auto tracking white balance, and auto focus functions can be set separately.

These menu items cannot be set when the thumbnail screen is displayed.

Item | Description of settings
--- | ---
[A.IRIS] | Enables/disables the auto iris control. [ON]: Performs the auto iris control operation when in auto mode. The <IRIS> button does not work. [OFF]: Auto iris control operation is not performed during auto mode. This activates the iris control selected with the <IRIS> button. Factory setting: [ON]
[AGC] | Sets the auto gain control operations when [ON] is selected in [A.IRIS]. [ON]: Performs the operation of the [AGC] function that automatically adjusts camera gain when in auto mode. [OFF]: Does not perform the operation of the [AGC] function that automatically adjusts camera gain when in auto mode. Factory setting: [ON]
[AGC LIMIT] | Sets the maximum gain value during [AGC] operation. [3dB], [6dB], [12dB], [18dB] Factory setting: [6dB]
[AGC POINT] | Sets the F value to switch control to [AGC] from auto iris during [AGC] operation. [F4.0], [F5.6] Factory setting: [F4.0]
[A.SHUTTER] | Sets the auto shutter control operations when [ON] is selected in [A.IRIS]. [ON]: Performs the operation of auto shutter when in auto mode. [OFF]: Does not perform the operation of auto shutter when in auto mode. Factory setting: [ON]
[A.SHUTTER LIMIT] | Sets the maximum shutter value during [A.SHUTTER] operation. [1/100], [1/120], [1/250] Factory setting: [1/250]
[A.SHUTTER POINT] | Sets the F value to switch control from auto iris to [A.SHUTTER] during [A.SHUTTER] operation. [F8.0], [F9.6] Factory setting: [F8.0]
[ATW] | Sets the operations of the auto tracking white balance function. [ON]: Activates the auto tracking white balance function when in auto mode. The [ATW] function cannot be switched between enabled and disabled with the <WHITE BAL> switch or USER buttons. However, if [ATW LOCK] is assigned to the USER button, the white balance value can be fixed with the USER button. [OFF]: [ATW] function operation is not performed in auto mode. Performs the operation of the white balance function selected with the <WHITE BAL> switch. Factory setting: [ON]
[AF] | Sets the operation of the auto focus. [ON]: Performs the operation of auto focus when in auto mode. The <FOCUS> switch does not work. [OFF]: Does not perform the operation of auto focus when in auto mode. Activates the focus function selected with the <FOCUS> switch. Factory setting: [ON]

Top of the page