- Top
- Menu Operations
- Menu list
- [NETWORK SETUP]

# [NETWORK SETUP]

Configure the settings regarding the network.

[4G/LTE PROPERTY] cannot be selected when the setting is not required on the connected 4G/LTE USB modem.

Item | Description of settings
--- | ---
[USB MODE SELECT] | Sets the camera operation mode when an external device is connected to the USB. [STORAGE]: Sets the mode to be used with connected devices such as an external hard disk drive. [DEVICE]: Selects the USB device mode for using P2 cards as mass storage, using computers or other devices connected via USB 2.0. Factory setting: [STORAGE]
[USB MODE] | Enables/disables the mode selected in [USB MODE SELECT]. [ON], [OFF] Factory setting: [OFF]
[NETWORK SEL] | Sets the connection method when connecting the camera with an external device (such as a computer) via network. [WLAN]: Connects via wireless LAN. [4G/LTE]: Connects via 3G/4G/LTE. [LAN]: Connects via the <LAN> terminal. [OFF]: Does not connect. Factory setting: [OFF]
[NETWORK FUNC] | [HTTP SERVER] | Configures the settings regarding the HTTP server. [BROWSE]: Enables the P2 browser function. [BROWSE (+CTRL)]: Enables the HTTP server function, starting and stopping recording at the terminal side, and preset control of time code or user bits. [DISABLE]:HTTP Disables the server function. Factory setting: [DISABLE]
| [PLAYLIST] | Sets entering/exiting of the playlist edit mode. [ON], [OFF] Factory setting: [OFF]
| [IP REMOTE] | Sets the remote control function using an IP connection. [ENABLE]: Enables remote control with IP connection. [DISABLE]: Disables remote control with IP connection. Factory setting: [DISABLE]
| [USER ACCOUNT] | Sets the user account name.
| [ACCOUNT LIST] | Displays the currently set user account name. Registering of new accounts, deleting accounts, or changing password can also be performed.
[FTP CLIENT SERVICE] | [SETTING DATA] | Sets the source from where client service settings are acquired. [INTERNAL]: Uses the settings set on the camera. [SD CARD]: Uses the settings of the file inside the SD memory card inserted in the SD card slot. When this item is set to [SD CARD], insert an SD memory card before turning on the power of the camera. Factory setting: [INTERNAL]
| [SERVER URL] | Sets the name or address of the destination server.
| [LOGIN USER] | Sets the login user ID.
| [LOGIN PASSWORD] | Sets the login password.
| [SSH] | Sets when transferring files using SSH. [ENABLE]: Uses SSH. [DISABLE]: Does not use SSH. Factory setting: [DISABLE]
| [SSH PORT] | Sets the network port number when SSH is used. Set the same number as the server. The menu setting value is displayed with []. Factory setting: [22]
| [LOAD (SD CARD)] | Loads the settings of the client service from the SD memory card.
| [SAVE (SD CARD)] | Saves the settings of the client service onto the SD memory card.
| [REC DURING UPLOAD] | Sets whether to use the rec during upload function. [ENABLE]: Uses the rec during upload function. [DISABLE]: Does not use the rec during upload function. Factory setting: [DISABLE]
| [AUTO COPY] | Sets whether to enable the function to register clips recorded using the camera automatically to the upload list when recording stops, and if enabled, sets the type of target clip. [REC CLIP(PROXY)]: Upload target is proxy data of recorded clips. [REC CLIP]: Upload target is recorded clips (main recording data and proxy data). [DISABLE]: Does not automatically upload recorded clips. Factory setting: [DISABLE]
| [UPLOAD LIST] | Displays the list information of clips to upload.
| [SAVE LOG (SD CARD)] | Save up to the latest 1000 logs for clip information (month and date, clip number (global clip ID), status) registered in the upload list to an SD memory card.
[STREAMING SETTING] | [START TRIGGER] | Sets the method for starting video streaming. [CAMERA]: Starts/stops streaming from the camera. [RECEIVER]: Operates the start/stop of the streaming distribution from the terminal on the network using the P2 Browser or the P2 Streaming Receiver. Factory setting: [RECEIVER]
| [SETTING DATA] | Sets the source from where settings for streaming is acquired when [CAMERA] is selected in [START TRIGGER]. [INTERNAL]: Uses the settings set on the camera. [SD CARD]: Uses the settings of the file inside the SD memory card inserted in the SD card slot. When this item is set to [SD CARD], insert an SD memory card before turning on the power of the camera. Factory setting: [INTERNAL]
| [SERVER ADDR.] | Sets the IP address of the device receiving the streaming video when [CAMERA] is selected in [START TRIGGER].
| [RTSP PORT] | Sets the RTSP port number required for streaming when [CAMERA] is selected in [START TRIGGER]. Factory setting: [554]
| [LOAD (SD CARD)] | When [CAMERA] is selected in [START TRIGGER] and [INTERNAL] is selected in [SETTING DATA], the connection information necessary for streaming distribution is read from the SD memory card.
| [SAVE (SD CARD)] | When [CAMERA] is selected in [START TRIGGER] and [INTERNAL] is selected in [SETTING DATA], the connection information necessary for streaming distribution is saved to the SD memory card.
| [START] | When [CAMERA] is selected in [START TRIGGER], the streaming distribution is started/stopped from the camera. [ON]: Starts streaming. [OFF]: Stops streaming.
[LAN PROPERTY] | [MAC ADDRESS] | Displays the MAC address of the <LAN> terminal on the camera. (Cannot be changed.)
| [DHCP] | Sets whether to use automatic acquisition via DHCP. (Mutually exclusive with [DHCP SERVER] setting) [ENABLE]: Uses automatic acquisition. [DISABLE]: Does not use automatic acquisition. Set [IP ADDRESS], [SUBNET MASK], [DEFAULT GATEWAY], [PRIMARY DNS], and [SECONDARY DNS]. Factory setting: [ENABLE]
| [IP ADDRESS] | Sets the IP address when [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.1]
| [SUBNET MASK] | Sets the subnet mask when [DISABLE] is selected in [DHCP]. Factory setting: [255.255.255.0]
| [DEFAULT GATEWAY] | Sets the default gateway when [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.254]
| [PRIMARY DNS] | Sets the primary DNS server when [DISABLE] is selected in [DHCP]. Factory setting: [0.0.0.0]
| [SECONDARY DNS] | Sets the secondary DNS server when [DISABLE] is selected in [DHCP]. Factory setting: [0.0.0.0]
| [DHCP SERVER] | Sets whether to use the DHCP SERVER function when connected via wired LAN. (Mutually exclusive with [DHCP] setting) [ENABLE]: Uses the DHCP SERVER function. [DISABLE]: Does not use the DHCP SERVER function. Factory setting: [DISABLE]
[WIRELESS PROPERTY] | [MAC ADDRESS] | Displays the MAC address of the wireless LAN of the camera. (Cannot be changed.)
| [TYPE] | Sets the connection method. [DIRECT]: Accesses to the network function of the camera directly from a smartphone, tablet, or computer. [INFRA]: Connects to the wireless access point. Factory setting: [DIRECT]
| [SSID INPUT MODE] | Sets the setting method of SSID. When [TYPE] in [WIRELESS PROPERTY] is set to [INFRA], this item can be set. [SELECT]: Selects from the access point list. [MANUAL]: For entering the access point manually. Factory setting: [SELECT]
| [SSID] | Displays network name (SSID).
| [BAND] | Switches between two transmission methods (2.4 GHz or 5 GHz). [2.4GHz], [5GHz] Factory setting: [2.4GHz]
| [CHANNEL (2.4GHz)] | Sets the channels to be used when [DIRECT] is selected in [TYPE], [2.4GHz] is selected in [BAND], and the camera is connected via wireless LAN. [AUTO], [CH1], [CH6], [CH11] Factory setting: [AUTO]
| [CHANNEL (5GHz)] | Sets the channels to be used when [DIRECT] is selected in [TYPE], [5GHz] is selected in [BAND], and the camera is connected via wireless LAN. The selections change according to the wireless module to mount. [AUTO], [CH36], [CH40], [CH44], [CH48], [CH149], [CH153], [CH157], [CH161], [CH165] Factory setting: [AUTO]
| [ENCRYPTION] | Sets the encryption format. [WPA-TKIP], [WPA-AES], [WPA2-TKIP], [WPA2-AES], [NONE] Factory setting: [WPA2-AES]
| [ENCRYPT KEY] | Sets the encryption key. Set the key using a string of 8 to 63 characters or a hexadecimal number with 64 digits. Factory setting: [01234567890123456789abcdef]
| [DHCP] | Sets whether to use automatic acquisition via DHCP when [INFRA] is selected in [TYPE]. [ENABLE]: Uses automatic acquisition. [DISABLE]: Does not use automatic acquisition. Set [IP ADDRESS], [SUBNET MASK], [DEFAULT GATEWAY], [PRIMARY DNS], and [SECONDARY DNS]. Factory setting: [ENABLE]
| [IP ADDRESS] | Sets the IP address when [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.1]
| [SUBNET MASK] | Sets the subnet mask when [DISABLE] is selected in [DHCP]. Factory setting: [255.255.255.0]
| [DEFAULT GATEWAY] | Sets the default gateway when [INFRA] is selected in [TYPE] and [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.254]
| [PRIMARY DNS] | Sets the primary DNS server when [INFRA] is selected in [TYPE] and [DISABLE] is selected in [DHCP], or when [ENABLE] is selected in [DHCP] and the primary DNS server cannot be obtained. Factory setting: [0.0.0.0]
| [SECONDARY DNS] | Sets the secondary DNS server when [INFRA] is selected in [TYPE] and [DISABLE] is selected in [DHCP], or when [ENABLE] is selected in [DHCP] and the primary DNS server cannot be obtained. Factory setting: [0.0.0.0]
| [DHCP SERVER] | Sets whether to use the DHCP SERVER function when [DIRECT] is selected in [TYPE] and the camera is connected via wireless LAN. [ENABLE]: Uses the DHCP SERVER function. [DISABLE]: Does not use the DHCP SERVER function. Factory setting: [ENABLE]
[4G/LTE PROPERTY] | [APN] | Sets the APN (Access Point Name) provided by the provider.
| [USER ID] | Sets the user name provided by the provider.
| [PASSWORD] | Sets the password provided by the provider.
| [DIAL NO.] | Sets the phone number. For details, refer to the manual of the provider you have contracted.
[NETWORK TOOLS] | [LOG DISPLAY] | Displays the connection log.
| [STATUS DISPLAY] | Displays the network status.
| [INITIALIZE] | Restores the network setting status to the factory settings.
| [PING] | Checks network connection using PING commands.

Top of the page