- Top
- Shooting
- Flash band compensation (FBC) function
- Setting the flash band compensation function

# Setting the flash band compensation function

Use after assigning the flash band compensation function to the USER button.

By pressing the USER button that is assigned with the flash band compensation function, the function turns on, and flash strobe from a still camera, etc. can be detected and compensated.

For details, refer to “Assigning functions to the USER buttons”.

When the flash band compensation function is enabled, [FBC] is displayed on the status screen.

NOTE

- When the flash strobe lights, the following phenomena may occur. These are due to the flash band compensation function and are not malfunctions.

  - Moving subjects look as if they have been stopped for a moment.

  - The resolution drops when the flash strobe lights.

  - Horizontal lines appear in the video when the flash strobe lights.

## Using the flash band compensation function

The flash band compensation function is activated when there are large changes in brightness at the bottom of the screen regardless of whether there is flash strobe light. The flash band compensation function may be activated depending on the shooting environment such as where a bright window has zoomed in and then out. So, we recommend use of this function in shooting environments where flash strobe lighting is anticipated.

Even if flash strobe lighting occurs, sufficient flash band compensation function effect may not be obtained in some shooting environments.

## Flash band compensation function operation conditions

- The conditions the flash band compensation function can be used in are 59.94i, 59.94P, 50i, or 50P mode and when the electronic shutter, digital zoom, and variable frame rate functions are not in operation.

- Even if the flash band compensation function is enabled, the flash band compensation function is forcibly disabled if the camera is changed to a mode where the flash band compensation function cannot be used.

  To use the function again, return to a mode where the function can be used, and press the USER button to turn on the flash band compensation function.

  The flash band compensation function is disabled once the power is turned off.

Top of the page