- Top
- Display
- Screen status display
- Checking and displaying shooting status

# Checking and displaying shooting status

Also, the mode check [STATUS] screen is displayed when the <DISP/MODE CHK> switch is pushed towards the <CHK> side. During mode check, almost all items are displayed including usually hidden items so that the shooting status can be checked. For details on the mode check, refer to “Mode check display”.

The list shows the display/hide status of each item in the [STATUS] screen. The display/hide status differ depending on the <DISP/MODE CHK> switch settings and settings in the main menu → [DISPLAY SETUP] → [OTHER DISPLAY].

- “✓” indicates displaying, and “—” indicates hiding.

- [ON]/[OFF] for each item can be selected in the main menu → [DISPLAY SETUP] → [DISPLAY SETTING].

No | Item | Shooting | Playback | <DISP/MODE CHK>: <CHK> | <DISP/MODE CHK>: <OFF> | <DISP/MODE CHK>: <ON>
--- | --- | --- | --- | --- | --- | ---
[OTHER DISPLAY]
[ALL] | [PARTIAL] | [USER]
1 | Time code display | ✓ | ✓ | —*1 | —*1 | —*1 | —*1 | —*1
2 | Shooting/recording and playback frame rate display | ✓ | ✓ | ✓ | — | ✓ | ✓ | ✓
3 | Proxy information display | ✓ | — | ✓ | —*2 | —*1 | —*1 | ✓
4 | SD memory card status display | ✓ | — | ✓ | —*2 | ✓ | ✓ | ✓
5 | System mode display | ✓ | ✓ | ✓ | — | ✓ | — | ✓
6 | Recording format display | ✓ | ✓ | ✓ | — | ✓ | — | ✓
7 | Letterbox recording display | ✓ | — | ✓ | — | ✓ | — | ✓
8 | Streaming mode setting status display | ✓ | — | ✓ | — | — | — | —
9 | Network information display | ✓ | — | ✓ | — | — | — | —
10 | Remote control display in an IP connection | ✓ | — | ✓ | — | — | — | —
11 | USER button information display | ✓ | — | —*1 | —*1 | —*1 | —*1 | —*1
12 | Focus bar display | ✓ | — | —*1 | —*1 | —*1 | —*1 | —*1
13 | Time stamp recording display | ✓ | — | ✓ | — | —*1 | —*1 | —*1
14 | Date and time display | ✓ | — | ✓ | — | —*1 | —*1 | —*1
15 | Audio level meter display | ✓ | ✓ | ✓ | — | —*1 | —*1 | —*1
16 | Audio recording not possible display | ✓ | — | ✓ | — | —*1 | —*1 | —*1
17 | Digital zoom display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
18 | Y GET brightness display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
19 | ND filter display | ✓ | — | ✓ | — | ✓ | — | ✓
20 | Shutter speed display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
21 | <WHITE BAL> switch position display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
22 | Auto iris control display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
23 | Gain display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
24 | Iris display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
25 | Zoom position display | ✓ | — | ✓ | — | —*1 | —*1 | —*1
26 | Focus control information display | ✓ | — | ✓ | — | —*1 | —*1 | —*1
27 | Macro display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
28 | Recommended ND filter display | ✓ | — | ✓ | — | ✓ | — | ✓
29 | Camera warning, notification display area | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓
30 | Area frame display | ✓ | — | —*1 | —*1 | —*1 | —*1 | —*1
31 | Area display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
32 | Flash band compensation function display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
33 | Dynamic range stretcher function display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
34 | Scene file name display | ✓ | — | ✓ | — | ✓ | — | ✓
35 | Image stabilization display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
36 | Battery charge level indicator | ✓ | ✓ | ✓ | —*2 | —*1 | —*1 | —*1
37 | P2 card remaining free space | ✓ | ✓ | ✓ | —*2 | —*1 | —*1 | —*1
38 | Recording media display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
39 | Simultaneous recording mode display | ✓ | — | ✓ | — | ✓ | — | ✓
Background recording mode display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
40 | High-sensitivity mode display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
41 | One clip recording mode status display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
42 | Rec during upload status and streaming distribution status display | ✓ | ✓ | — | — | —*1 | —*1 | —*1
43 | Recording/playback operation status display | ✓ | ✓ | ✓ | —*3 | ✓ | ✓ | ✓
44 | <AUTO/MANUAL> switch operation display | ✓ | — | ✓ | — | ✓ | ✓ | ✓
45 | GPS display | ✓ | — | ✓ | — | ✓ | — | ✓
46 | 4G/LTE connection status and the bonding device status display | ✓*4 | — | ✓*4 | — | ✓*4 | ✓*4 | ✓*4
47 | HD SDI REMOTE recording status display | ✓*4 | — | ✓*4 | — | ✓*4 | ✓*4 | ✓*4
48 | Audio monitor volume adjustment display | ✓ | ✓ | —*1 | —*1 | —*1 | —*1 | —*1
49 | Front audio level volume display | ✓ | — | —*1 | —*1 | —*1 | —*1 | —*1

May be displayed depending on other settings.

Displayed when the remaining capacity becomes smaller.

Displayed during shooting.

Always displayed when 4G/LTE connection is set, bonding device is connected, and [HD SDI REMOTE] setting is set.

Top of the page